[Contents] [Prev] [Next] [Index] [Report an Error]

## Creating and Attaching a Policy with IP Classifiers

In this example, a policy with a combination of IP classifiers is created and attached. The configuration conforms to the 128 bit limit.

1. Match all TCP SYN packets from 1.1.1.1 to any DA with port 2000.
   `
   host1(config)#ip classifier-list tcpCLACL tcp host 1.1.1.1 any eq 2000 tcp-flags "SYN"
   `
2. Match all IP packets with the don’t fragment flag set to host 2.2.2.2.
   `
   host1(config)#ip classifier-list ipCLACL ip any host 2.2.2.2 ip-flags "dont-fragment"
   `
3. Match all ICMP echo packets.
   `
   host1(config)#ip classifier-list icmpCLACL icmp any any 8 0
   `
4. Match all frames with the color red.
   `
   host1(config)#ip classifier-list colorCLACL color red ip any any
   `
5. Create a policy list.
   `
   host1(config)#ip policy-list ipPol
   host1(config-policy-list)#classifier-group colorCLACL
   host1(config-policy-list-classifier-group)#filter
   host1(config-policy-list-classifier-group)#classifier-group tcpCLACL
   host1(config-policy-list-classifier-group)#filter
   host1(config-policy-list-classifier-group)#classifier-group icmpCLACL
   host1(config-policy-list-classifier-group)#filter
   host1(config-policy-list-classifier-group)#classifier-group ipCLACL
   host1(config-policy-list-classifier-group)#filter
   `
6. Apply the policy list to an interface.
   `
   host1(config)#interface atm 5/0.1
   host1(config-if)#ip policy input ipPol
   `

   Table 23 lists the active classifiers in the policy named ipPol and the size of each classifier.

   Table 23: Classification Fields for Example 1

   Classifiers | Size (Bits)
   --- | ---
   Source address | 32
   Destination address | 32
   Destination port, ICMP type, ICMP code | 16
   Protocol | 8
   Color and TCP flags | 8
   TOS | 8
   IP flags | 8

   The total value of the classifiers requested in the ipPol policy is 112, which is less than 128 bit CAM entry size limit.

In this example, a policy with a combination of IP classifiers is created and attached. The configuration exceeds the 128 bit limit.

1. Match all TCP packets from 1.1.1.1 port 10 to 2.2.2.2 port 20.
   `
   host1(config)#ip classifier-list tcpCLACL tcp host 1.1.1.1 eq 10 host 2.2.2.2 eq 20
   `
2. Match all IP fragmentation offset equal to 1.
   `
   host1(config)#ip classifier-list ipFragCLACL ip any any ip-frag-offset eq 1
   `
3. Match all frames with the color red.
   `
   host1(config)#ip classifier-list colorCLACL color red traffic-class best-effort ip any any
   `
4. Match all frames with UPC 1.
   `
   host1(config)#ip classifier-group upcCLACL user-packet-class 1 ip any any
   `
5. Create a policy list.
   `
   host1(config)#ip policy-list ipPol
   host1(config-policy-list)#classifier-group colorCLACL
   host1(config-policy-list-classifier-group)#filter
   host1(config-policy-list-classifier-group)#classifier-group ipFragCLACL
   host1(config-policy-list-classifier-group)#filter
   host1(config-policy-list-classifier-group)#classifier-group igmpCLACL
   host1(config-policy-list-classifier-group)#forward
   host1(config-policy-list-classifier-group)#classifier-group lowDelayCLACL
   host1(config-policy-list-classifier-group)#traffic-class strict-priority
   host1(config-policy-list-classifier-group)#classifier-group tcpCLACL
   host1(config-policy-list-classifier-group)#forward
   host1(config-policy-list-classifier-group)#classifier-group *
   host1(config-policy-list-classifier-group)#filter
   `
6. Apply the policy list to an interface.
   `
   host1(config)#interface atm 5/0.1
   host1(config-if)#ip policy input ipPol
   % too many classifier fields in policy
   `

   Table 24 lists the active classifiers in the policy named ipPol and the size of each classifier.

   Table 24: Classification Fields for Example 2

   Classifiers | Size (Bits)
   --- | ---
   Source address | 32
   Source port | 16
   Destination port | 16
   Protocol | 8
   User packet class | 8
   Color | 8
   IP fragmentation | 8
   ToS | 8

   The configuration fails because the total value of the classifiers requested in the ipPol policy is 136, which is greater than 128 bit CAM entry size limit.

[Contents] [Prev] [Next] [Index] [Report an Error]