[Contents] [Prev] [Next] [Index] [Report an Error]

# show ip bgp community-list

#### Syntax

show ip bgp [ ipv4 unicast | ipv4 multicast | vpnv4 all | vpnv4 vrf vrfName |
l2vpn all | l2vpn vpls vplsName | l2vpn vpws vpwsName | route-target signaling ]
community-list communityListName [ exact-match ] [ fields fieldOptions ] [ filter ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.
l2vpn and all keywords added in JUNOSe Release 7.1.0.
vpls keyword and vplsName variable added in JUNOSe Release 7.1.0.
vpws keyword and vpwsName variable added in JUNOSe Release 8.1.0.
route-target signaling keywords added in JUNOSe Release 8.2.0.

#### Description

Displays routes that belong to the BGP community specified by the community list.

#### Options

- ipv4 unicast—Specifies the IPv4 unicast address family and routing table; the default option
- ipv4 multicast—Specifies the IPv4 multicast address family and routing table
- vpnv4 all—Specifies the IPv4 VPN address family and all IPv4 VPN routing and forwarding instances
- vpvn4 vrf vrfName—Specifies the IPv4 VPN address family and only the IPv4 VPN routing and forwarding instance with the name vrfName
- l2vpn all—Specifies all VPLS and VPWS instances in the L2VPN address family
- l2vpn vpls vplsName—Specifies the VPLS instance with the name vplsName
- l2vpn vpws vpwsName—Specifies the VPWS instance with the name vpwsName
- route-target signaling—Specifies the route-target address family
- communityListName—Filters routes according to community list; displays only routes that are members of a community on the specified list
- exact-match—Displays only routes that have exactly the specified communities
- fields—Displays only the specified fields; the display order of the fields is hard-coded and not affected by the order in which you enter them
- fieldOptions—Fields to be displayed, in the format
  all | [ afi | aggregator | as-path | atomic-aggregate | best | clusters | communities | extended-communities | imported | intro | in-label | loc-pref | med | next-hop | next-hop-cost | origin | originator-id | out-label | peer | peer-type | rd | safi | stale | unknown-types | weight ]*
  - all—All available information; not recommended, because this information for each network does not fit on a single line and is difficult to read
  - afi—Address family identifier
  - aggregator—AS number and IP address of aggregator
  - as-path—AS path through which this route bas been advertised
  - atomic-aggregate—Whether the atomic aggregate attribute is present
  - best—Whether this is the best route for the prefix
  - clusters—List of cluster IDs through which the route has been advertised
  - communities—Community number associated with the route
  - extended-communities—Extended community
  - imported—Whether the route was imported
  - intro—Introductory information about the state of various BGP attributes; this information is displayed only if you specify this keyword
  - in-label—MPLS label for the route; the label received with incoming MPLS frames; typically, but not always, this is the label advertised to MP-BGP peers
  - loc-pref—Local preference for the route
  - med—Multiexit discriminator for the route
  - next-hop—IP address of the next router that is used when forwarding a packet to the destination network
  - next-hop-cost—Whether the indirect next hop of the route is unreachable, if not, displays IGP cost to the indirect next hop
  - origin—Origin of the route
  - originator-id—Router ID of the router in the local AS that originated the route
  - out-label—MPLS label for the route; the label sent with outgoing MPLS frames; also the label received from MP-BGP peer; typically, but not always, this is the label received from MP-BGP peers
  - peer—IP address of BGP peer from which route was learned
  - peer-type—Type of BGP peer: internal, external, or confederation
  - rd—Route distinguisher
  - safi—Subsequent address family identifier
  - stale—Route that has gone stale due to peer restart
  - unknown-types—Attribute codes for unknown path attributes
  - weight—Weight of the route
  - *—Indicates that one or more parameters can be repeated multiple times in a list in the command line
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec

#### Related Topics

- Monitoring BGP-Related Settings for L2VPNs in the JUNOSe BGP and MPLS Configuration Guide

[Contents] [Prev] [Next] [Index] [Report an Error]