[Contents] [Prev] [Next] [Index] [Report an Error]

# bulkstats interface-type

#### Syntax

[ no ] bulkstats interface-type interfaceType [ interfaceSpecifier ]*
[ collector collectorIndex ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.
mplsL2shim, mplsMajor, and mplsMinor keywords added in JUNOSe Release 8.2.0.

#### Description

Configures the interface type on which you want to collect statistics. The no version deletes the interface type from bulkstats collection.

#### Options

- interfaceType—One of the following interface types for which you can collect statistics: ATM, ATM 1483, Ethernet, Frame Relay, Frame Relay subinterface, Cisco HDLC, IP, MPLS minor, MPLS major, MPLS shim, PPP, VLAN subinterface
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- *—Indicates that one or more parameters can be repeated multiple times in a list in the command line
- collectorIndex—Number in the range 1–65535 that identifies the particular data collector. Always specify this option if you defined more than one collector.

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]