[Contents] [Prev] [Next] [Index] [Report an Error]

# frame-relay lmi-n393dte

#### Syntax

frame-relay lmi-n393dte events

no frame-relay lmi-n393dte

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Sets the monitored event count (N393) on a DTE interface. The no version removes current setting and sets the default.

#### Options

- events—Number in the range 1–10 events; default value is 4 events; specifies the diagnostic window used to verify link integrity (the detection of N392 errors within the window of N393 samples places the interface in an operationally down state)

#### Mode

Interface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]