[Contents] [Prev] [Next] [Index] [Report an Error]

# ip flow-cache entries

#### Syntax

ip flow-cache entries cacheEntries

no ip flow-cache entries

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Limits the number of entries in the flow cache (for all line modules in the router). The no version sets the number of entries back to its default value.

#### Options

- cacheEntries—Number of cache entries allowed for all line modules in the router in the range 1024–524288; default value is 65536

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]