[Contents] [Prev] [Next] [Index] [Report an Error]

# enable ipsec-transport

#### Syntax

[ no ] enable ipsec-transport

#### Release Information

Command introduced before JUNOSe Release 7.1.0.
IP Tunnel Destination Profile Configuration mode added in JUNOSe Release 8.2.0.

#### Description

In IP Tunnel Destination Profile Configuration mode, specifies that the router accepts only dynamic IP tunnels protected by an IPSec transport connection. The no version disables IPSec transport mode.

In L2TP Destination Profile Host Configuration mode, specifies that the router accepts only L2TP tunnels protected by an IPSec transport connection. The no version disables IPSec transport mode.

#### Mode

IP Tunnel Destination Profile Configuration, L2TP Destination Profile Host Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]