[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring Configuration, Statistics, and Status for VPLS Network Interfaces

Purpose

Display configuration, statistics, and status information for a specified network interface or for all interfaces assigned to a VPLS instance.

Action

To display information for a specified network interface:

    host1#show bridge interface atm 3/1.10

        atm3/1.10
          BridgeGroup: vplsB
          Port Number: 1
          Operational Status: Up
          Admin Status: Up
          Snmp Link Status Trap: Disabled
          Max Learn: Unlimited
          Subscriber Policy: default Trunk
          Statistics:
             In Octets:    1958
             In Frames:    14
             In Discards:  1
             In Errors:    0
             Out Octets:   1930
             Out Frames:   14
             Out Discards: 1
             Out Errors:   0
          Time since counters last reset: 00:14:32

          queue 0: traffic class best-effort, bound to bridge ATM3/1.10
            Queue length 0 bytes
            Forwarded packets 14, bytes 2238
            Dropped committed packets 0, bytes 0
            Dropped conformed packets 0, bytes 0
            Dropped exceeded packets 0, bytes 0

To display information about all interfaces in a VPLS instance, including the VPLS virtual core interface (vplsB):

    host1#show bridge vplsB interface

        FastEthernet1/1.1
          Port Number: 1
          Operational Status: Up
          Admin Status: Up
          Snmp Link Status Trap: Disabled
          Max Learn: Unlimited
          Subscriber Policy: samplepolicy
          Statistics:
             In Octets:    3770
             In Frames:    27
             In Discards:  0
             In Errors:    0
             Out Octets:   3682
             Out Frames:   27
             Out Discards: 0
             Out Errors:   0
          Time since counters last reset: 01:07:08

          queue 0: traffic class best-effort, bound to bridge FastEthernet1/1.1
            Queue length 0 bytes
            Forwarded packets 27, bytes 3898
            Dropped committed packets 0, bytes 0
            Dropped conformed packets 0, bytes 0
            Dropped exceeded packets 0, bytes 0

        vpls vplsB
          Port Number: 2
          Operational Status: Down
          Admin Status: Up
          Snmp Link Status Trap: Disabled
          Max Learn: Unlimited
          Subscriber Policy: default Trunk
          Statistics:
             In Octets:    0
             In Frames:    0
             In Discards:  0
             In Errors:    0
             Out Octets:   0
             Out Frames:   0
             Out Discards: 40
             Out Errors:   0
          Time since counters last reset: 01:04:10

To display a summary of all interfaces configured for the specified VPLS instance:

    host1#show bridge vplsB interface brief
            Interface            Port       Status
    -------------------------   ------   ------------
    FastEthernet1/1.1           1        Up
    ATM10/1.1.1                 2        Up
    vpls vplsB                  3        Up

Meaning

Table 86 lists the show bridge interface command output fields.

Table 86: show bridge interface Output Fields

Field Name | Field Description
--- | ---
BridgeGroup | Name of the VPLS instance to which the interface belongs
Port Number | Port number on which this interface resides
Operational Status | Operational status of the physical interface: Up, Down, LowerLayerDown, NotPresent
Admin Status | State of the physical interface: Up, Down
Snmp Link Status Trap | Whether SNMP link status processing is enabled or disabled for the specified interface
Max Learn | Maximum number of dynamic MAC addresses that the interface can learn
Subscriber Policy | Name of the subscriber policy currently in effect for the interface
Statistics | Displays statistics information for the specified port
In Octets | Number of octets received on this interface
In Frames | Number of frames received on this interface
In Discards | Number of incoming packets discarded on this interface
In Errors | Number of incoming errors received on this interface
Out Octets | Number of octets transmitted on this interface
Out Frames | Number of frames transmitted on this interface
Out Discards | Number of outgoing packets discarded on this interface
Out Errors | Number of outgoing errors on this interface
Time since counters last reset | Elapsed time since statistics counters were last reset
queue | Hardware packet queue associated with the specified traffic class and interface
Queue length | Length of the queue, in bytes
Forwarded packets, bytes | Number of packets and bytes forwarded on this queue
Dropped committed packets, bytes | Number of committed packets and bytes that were dropped
Dropped conformed packets, bytes | Number of conformed packets and bytes that were dropped
Dropped exceeded packets, bytes | Number of exceeded packets and bytes that were dropped
vpls vplsName | Identifies the VPLS virtual core interface for the VPLS instance

Table 87 lists the show bridge interface brief command output fields.

Table 87: show bridge interface Output Fields

Field Name | Field Description
--- | ---
Interface | Interface type and specifier associated with the port
Port | Port number on which this interface resides
Status | Operational status of the physical interface: Up, Down, LowerLayerDown, NotPresent

#### Related Topics

- show bridge interface

[Contents] [Prev] [Next] [Index] [Report an Error]