[Contents] [Prev] [Next] [Index] [Report an Error]

# auto-configure vlan

#### Syntax

[ no ] auto-configure vlan

#### Release Information

Command introduced in JUNOSe Release 7.1.0.

#### Description

Configures the static VLAN major interface to support autodetection of a dynamic VLAN subinterface. The no version terminates autodetection of the VLAN subinterface.

#### Mode

Interface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]