[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring Detailed Configuration Information about Specified Sessions

#### Purpose

Display detailed configuration information about specified sessions.

#### Action

To display detailed configuration information about specified sessions:

To display L2TP session:

    host1#show l2tp session
    L2TP session 1/1/1 is Up
    1 L2TP session found

To display L2TP session details:

    host1#show l2tp session detail
    L2TP session 1/1/1 is Up
    Configuration
      Administrative state is enabled
      SNMP traps are enabled
    Session status
      Effective administrative state is enabled
      State is established
      Local session id is 25959, peer session id is 2
    Statistics packets octets discards errors
      Data rx  7       237    1        0
      Data tx  6       160    0        0

    Session operational configuration
      User name is 't1.s1@local'
      Tunneling PPP interface atm 0/0.1
      Call type is lacIncoming
      Call serial number is 0
      Bearer type is none
      Framing type is none
      Proxy LCP was provided
      Authentication method was chap
      Tunnel switch profile is chicago

#### Meaning

Table 88 lists the show l2tp session command output fields.

Table 88: show l2tp session Output Fields

Field Name | Field Description
--- | ---
Configuration | Configured status of the session
Administrative state | Administrative status of the destination: enabled—No restrictions on the operation of this session disabled—Router terminated this session
SNMP traps | Whether or not the router sends traps to Simple Network Management Protocol (SNMP) for operational state changes
Session status | Session status of the destination
Effective administrative state | Most restrictive of the following administrative states: router, destination, tunnel, and session. This setting, rather than the administrative state of the session, determines whether the router can maintain this session or not.
State | Status of the session: idle, connecting, established, or disconnecting
Local and peer session id | Names the router uses to identify the session locally and remotely
Statistics | Information about the traffic for this session
Session operational configuration | Information received from the peer when the session was created

#### Related Topics

- show l2tp session

[Contents] [Prev] [Next] [Index] [Report an Error]