[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring the QoS Configuration of Fast Ethernet, Gigabit Ethernet, and 10-Gigabit Ethernet Interfaces

#### Purpose

Display information about the QoS configuration for a specific Fast Ethernet, Gigabit Ethernet, or 10-Gigabit Ethernet interface.

#### Action

To display the QoS configuration for a Fast Ethernet interface:

    host1#show interfaces fastEthernet 6/0
    GigEthernet6/0 is Up, Administrative status is Up
    Hardware is Intel 21440, address is 0090.1a40.5508
    MAU is 100BASE-TX
    MTU: Operational 1522, Administrative 1522
    Duplex Mode: Operational Full Duplex, Administrative Auto Negotiate
    Speed: Operational 100 Mbps, Administrative Auto Negotiate
    5 minute input rate 0 bits/sec, 0 packets/sec
    5 minute output rate 0 bits/sec, 0 packets/sec
    In: Bytes 0, Unicast 0
    Multicast 0, Broadcast 0
    Errors 0, Discards 0, Mac Errors 0, Alignment 0
    CRC 0, Too Longs 0, Symbol Errors 0
    Out: Bytes 64, Unicast 0
    Multicast 0, Broadcast 1
    Errors 0, Discards 0, Mac Errors 0, Deferred 0, No Carrier 0
    Collisions: Single 0, Multiple 0, Late 0, Excessive 0
    Administrative qos-shaping-mode: cell
    Operational qos-shaping-mode: cell
    Attached QoS profile: ss

To display the QoS configuration for a Gigabit Ethernet interface:

    host1#show interfaces gigabitEthernet 2/0

To display the QoS configuration for a 10-Gigabit Ethernet interface:

    host1#show interfaces tenGigabitEthernet 5/0/0

#### Meaning

Table 51 lists the related show interfaces command output fields.

Table 51: show interfaces Output Fields

Field Name | Field Description
--- | ---
Administrative qos-shaping-mode | QoS shaping mode: disabled frame cell none
Operational qos-shaping-mode | QoS shaping mode: disabled frame cell none
Attached QoS profile | QoS profile attachment at or below the displayed interface. For example, if the interface being displayed is a VLAN subinterface, and the attachment is at the Gigabit Ethernet interface, the Gigabit Ethernet attachment is displayed.

#### Related Topics

- Configuring the QoS Shaping Mode for Ethernet Interfaces
- Creating Parameter Instances
- For more information about other fields displayed with this command, see JUNOSe Physical Layer Configuration Guide
- show interfaces command

[Contents] [Prev] [Next] [Index] [Report an Error]