[Contents] [Prev] [Next] [Index] [Report an Error]

# tunnel mpls no-route retries

#### Syntax

tunnel mpls no-route retries retryNum

no tunnel mpls no-route retries

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies for a particular tunnel the number of attempts that will be made to set up an LSP for RSVP-TE after a failure due to no available route. The no version restores the default value, 0, which means the attempts will be made until successful.

#### Options

- retryNum—Number of retry attempts in the range 0–65535

#### Mode

Interface Configuration, Tunnel Profile Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]