[Contents] [Prev] [Next] [Index] [Report an Error]

# pppoe remote-circuit-id

#### Syntax

[ no ] pppoe remote-circuit-id

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Enables a static or dynamic PPPoE interface on the router to capture and process a vendor-specific tag containing a remote circuit ID transmitted from a DSLAM device. The router can then send this value to a RADIUS server or to an L2TP network server (LNS) to uniquely identify subscriber locations. The no version restores the default behavior, which is not to capture and process the remote circuit ID.

#### Mode

Interface Configuration, Profile Configuration, Subinterface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]