[Contents] [Prev] [Next] [Index] [Report an Error]

# lsp-gen-interval

#### Syntax

lsp-gen-interval [ level-1 | level-2 ] seconds

no lsp-gen-interval [ level-1 | level-2 ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Sets the minimum interval at which originated IS-IS link-state packets are generated on a per LSP basis. The no version restores the default value, 5 seconds.

#### Options

- level-1—Sets interval for level 1 only
- level-2—Sets interval for level 2 only
- seconds—Number in the range 0–120; the minimum interval in seconds; default value is 5 seconds

#### Mode

Router Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]