[Contents] [Prev] [Next] [Index] [Report an Error]

# show radius remote-circuit-id-format

#### Syntax

show radius remote-circuit-id-format

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Displays the format of the PPPoE remote circuit ID value sent from a DSLAM and captured on the router.

If the PPPoE remote circuit ID value is configured to include any or all of the agent-circuit-id, agent-remote-id, and nas-identifier components, the display lists the components included and the order in which they appear.

If the PPPoE remote circuit ID value is configured to use the format for the dsl-forum-1 keyword of the radius remote-circuit-id-format command, the display indicates that this format is in effect.

#### Mode

Privileged Exec

[Contents] [Prev] [Next] [Index] [Report an Error]