[Contents] [Prev] [Next] [Index] [Report an Error]

# debug ip rip

#### Syntax

debug ip rip ripLog [ severity { severityValue | severityNumber } ]
[ verbosity verbosityLevel ]

no debug ip rip ripLog

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Shows information about the selected variable. The no version disables the display.

#### Options

- ripLog—RIP log of interest; one of the following options:
  - events—General RIP events, such as removing RIP from an interface or creating the RIP process
  - route—Events associated with two RIP routers exchanging routes
- severity—Specifies the minimum severity of the log messages displayed for the selected category; described either by a descriptive term—severityValue—or by a corresponding number—severityNumber—in the range 0–7; the lower the number, the higher the priority:
  - emergency or 0—System unusable
  - alert or 1—Immediate action needed
  - critical or 2—Critical condition exists
  - error or 3—Error condition
  - warning or 4—Warning condition
  - notice or 5—Normal but significant condition
  - info or 6—Informational message
  - debug or 7—Debug message
- verbosityLevel—Verbosity of the log category's messages; can be any of the following:
  - low—Terse
  - medium—Moderate detail
  - high—Verbose

#### Mode

Privileged Exec

[Contents] [Prev] [Next] [Index] [Report an Error]