[Contents] [Prev] [Next] [Index] [Report an Error]

## Index

Symbols A B C D E F G H I K L M N O P Q R S T U V W

Symbols

> 10-Gigabit Ethernet interfaces 1
>   specifying an interface 1

A

> AAA (authentication, authorization, accounting) 1
>   DSL Forum VSAs 1
>   EAP authentication 1
>   failure, notifying RADIUS of 1
>   L2TP tunnel switch profiles, applying 1
>   overview 1
>   services 1
>     accounting 1
>     and TACACS+ 1
>     authentication 1
>     authorization 1
>     overview 1
> aaa commands 1
>   aaa accounting acct-stop on-aaa-failure 1
>   aaa accounting acct-stop on-access-deny 1
>   aaa accounting broadcast 1
>   aaa accounting commands 1
>   aaa accounting default 1
>   aaa accounting duplication 1
>   aaa accounting exec 1
>   aaa accounting immediate-update 1
>   aaa accounting interval 1
>   aaa accounting statistics 1
>   aaa accounting suppress null-username 1
>   aaa accounting tacacs+ 1
>   aaa accounting vr-group 1
>   aaa authentication default 1
>   aaa authentication enable default 1
>   aaa authentication login 1
>   aaa delimiter 1
>   aaa dhcpv6-delegated-prefix delegated-ipv6-prefix 1
>   aaa dns primary 1
>   aaa dns secondary 1
>   aaa domain-map 1
>   aaa duplicate-address-check 1
>   aaa intf-desc-format include 1
>   aaa ipv6-nd-ra-prefix framed-ipv6-prefix 1
>   aaa local database 1
>   aaa local select database 1
>   aaa local username 1
>   aaa new-model 1
>   aaa parse-direction 1
>   aaa parse-order 1
>   aaa profile 1
>   aaa route-download 1
>   aaa route-download now 1
>   aaa route-download suspend 1
>   aaa service accounting interval 1
>   aaa subscriber limit per-port 1
>   aaa subscriber limit per-vr 1
>   aaa timeout 1
>   aaa tunnel assignment-id-format 1
>   aaa tunnel calling-number-format 1
>   aaa tunnel calling-number-format fallback 1
>   aaa tunnel client-name 1
>   aaa tunnel ignore 1
>   aaa tunnel password 1
>   aaa tunnel switch-profile 1
>   aaa tunnel tx-connect-speed-method 1
>   aaa tunnel-group 1
>   aaa user accounting interval 1
>   aaa virtual-router 1
>   aaa wins primary 1
>   aaa wins secondary 1
>   See also
> AAA default tunnel parameters 1
>   L2TP transmit connect speed 1
> AAA domain maps 1
>   configuring 1
>     IPv6 local address pools 1
>   IPv6 local address pools 1
>     and Prefix Delegation 1
>     overriden by pools in Access-Accept message 1
>   L2TP transmit connect speed 1
>   preference order 1
>     for determining local address pools 1
>   tunnel subscribers 1
> AAA LLID (logical line identifier) 1
>   configuration steps 1
>   how it works 1
>   monitoring 1
>   preauthentication considerations 1
>   RADIUS attributes in preauthentication request 1
>   troubleshooting 1
>   using to track subscribers 1
> AAA logical line identifier (LLID). 1, See AAA LLID
> AAA profile commands 1
>   aaa profile 1
>   allow 1
>   deny 1
>   nas-port-type atm 1
>   nas-port-type ethernet 1
>   ppp aaa-profile 1
>   service-description 1
>   translate 1
> AAA profiles 1
>   allowing or denying domain names 1
>   configuring 1
>   creating domain name aliases 1
>   manually setting NAS-Port-Type 1
>   setting Service-Description 1
> AAA tunnel groups 1
>   L2TP transmit connect speed 1
> Access-Accept messages 1
>   pool or prefix name 1
>     not available in 1
>   preference order 1
>     in allocation of IPv6 prefixes 1
>   RADIUS attribute used in 1
>     Prefix Delegation 1
>   with Framed-IPv6-Prefix attribute 1
>     for Prefix Delegation 1
>   with IPv6-NdRa-Prefix attribute 1
>     for IPv6 Neighbor Discovery 1
> Access-Challenge messages 1
> Access-Reject messages 1
> Access-Request messages 1
>   ANCP (L2C)-related VSAs 1
>   DSL Forum VSAs 1
> accounting 1
>   broadcast 1
>   configuring servers 1
>   configuring TACACS+ 1
>   description 1
>   duplicate 1
>   server access 1
>   server request processing limit 1
>   SNMP traps 1
>   specifying methods 1
>   TACACS+ 1
> accounting statistics 1
>   tunneled PPP session 1
> Acct-Authentic (RADIUS attribute 45) 1
> Acct-Delay-Time (RADIUS attribute 41) 1
> Acct-Input-Gigapackets (RADIUS attribute 26-35) 1
> Acct-Input-Gigawords (RADIUS attribute 52) 1
> Acct-Link-Count (RADIUS attribute 51) 1
> Acct-Multi-Session-Id (RADIUS attribute 50) 1
> Acct-Off messages 1
> Acct-On messages 1
> Acct-Output-Gigapackets (RADIUS attribute 26-36) 1
> Acct-Session-Id (RADIUS attribute 44) 1
> Acct-Start messages 1
>   ANCP (L2C)-related VSAs 1
>   DSL Forum VSAs 1
> Acct-Stop messages 1
>   ANCP (L2C)-related VSAs 1
>   DSL Forum VSAs 1
> Acct-Terminate-Cause (RADIUS attribute 49) 1
> Acct-Tunnel-Connection (RADIUS attribute 68) 1
> Activate-Service (RADIUS attribute 26-65) 1
> address command, L2TP 1
> address pool 1
>   mapping to domain name 1
>   ranges 1
> address-pool-name command 1
> agent circuit ID (suboption 1) 1
> agent remote ID (suboption 2) 1
> agent-circuit-id 1
>   including in Calling Number AVP 1
>   including in PPPoE remote circuit ID format 1
> agent-remote-id 1
>   including in Calling Number AVP 1
>   including in PPPoE remote circuit ID format 1
> allow command 1
> Ascend-Num-In-Multilink (RADIUS attribute 188) 1
> ATM (Asynchronous Transfer Mode) 1
>   E120 and E320 routers 1
> atm atm1483 advisory-rx-speed command 1
>   and L2TP 1
> atm commands 1
>   atm 1
>   atm pvc 1
> ATM subinterface 1
>   configuring multiple clients 1
>   configuring single clients 1
> attribute value pair. 1, See AVP
> authentication 1
>   AAA overview 1
>   configuring servers 1
>   configuring TACACS+ 1
>   description 1
>   EAP 1
>   preauthenticating users 1
>   redirected authentication 1
>   server access 1
>   server request processing limit 1
>   SNMP traps 1
>   specifying methods 1
> authentication and accounting servers 1
>   configuring 1
> authentication login, TACACS+ 1
> authentication, authorization, accounting. 1, See AAA
> authorization 1
>   AAA overview 1
>   description 1
>   TACACS+ 1
> authorization change command 1
> AVP (attribute value pair) 1
>   Bearer Type (AVP 18) 1
>     relaying in L2TP tunnel-switched network 1
>     relaying in L2TP tunnel-switchednetwork 1
>   Calling Number (AVP 22) 1
>     formatting and preventing in ICRQ packets 1
>     relaying in L2TP tunnel-switched network 1
>     relaying in L2TP tunnel-switchednetwork 1
>   Cisco NAS Port Info (AVP 100) 1
>     relaying in L2TP tunnel-switched network 1
>     relaying in L2TP tunnel-switchednetwork 1
>   Transmit (TX) Speed (AVP 24) 1
>     reporting transmit connect speed in 1
> avp command 1

B

> B-RAS applications 1
>   AAA profiles 1
>   allowing or denying domain names 1
>   client to server interaction 1
>   configuring 1
>     authentication and accounting servers 1
>     B-RAS license 1
>     DHCP external server application 1
>     DHCP features 1
>     IP addresses for remote clients 1
>     local address servers 1
>     name server addresses 1
>     SRC client 1
>     timeout 1
>     UDP checksums 1
>   creating an IP interface 1
>   creating domain name aliases 1
>   DHCP (Dynamic Host Configuration Protocol) proxy client and server 1
>   IP hinting 1
>   limiting active subscribers 1
>   local address server 1
>   manually setting NAS-Port-Type 1
>   mapping address pool to domain 1
>   mapping backup address pool to domain 1
>   mapping IPv6 local address pool to domain 1
>   mapping user domain names to a virtual router 1
>   mapping user requests 1
>     without a valid domain name 1
>     without configured domain name 1
>   monitoring 1
>   multiple clients per ATM subinterface 1
>   overview 1
>   preauthenticating users 1
>   protocol support 1
>   redirected authentication 1
>   references 1
>   setting Service-Description 1
>   single clients per ATM subinterface 1
>   SNMP traps 1
>   specifying a single name for a domain 1
>   SRC client. 1, See SRC software
>   system log messages 1
>   virtual router 1
> B-RAS licenses 1
>   configuring 1
> backoff algorithm 1
> backup address pool 1
>   mapping to domain name 1
> backup local address pool 1
>   and dependency on primary address pool 1
> backup-address-pool-name command 1
> baseline commands 1
>   baseline aaa 1
>   baseline aaa route-download 1
>   baseline cops 1
>   baseline dhcp relay 1
>   baseline dhcp server 1
>   baseline dhcp-local 1
>   baseline dhcpv6-local 1
>   baseline ip dhcp-external 1
>   baseline ip http 1
>   baseline local pool 1
>   baseline radius 1
>   baseline radius dynamic-request 1
>   baseline radius relay 1
>   baseline sscc 1
> Bearer Type AVP 1
>   relaying in L2TP tunnel-switched network 1
> BOOTP (bootstrap protocol) 1
> bootstrap protocol. 1, See BOOTP
> bridged Ethernet and dynamic subscriber interfaces 1
> Broadband Remote Access Server. 1, See B-RAS applications
> broadcast AAA accounting 1
>   configuring 1
> broadcast flag, DHCP 1
>   controlling transmission of DHCP reply packets 1
>   interaction with layer 2 unicast transmission method 1
> bundled session commands 1
>   bundled-group-id 1
>   bundled-group-id-overrides-mlppp-ed 1
> bundled sessions 1

C

> cable modem DHCP relay 1
> cable modem networks 1
> Called-Station-Id (RADIUS attribute 30) 1
> Calling Number AVP 1
>   descriptive formats 1
>   fixed format 1
>   fixed format configuration 1
>   formatting in L2TP ICRQ packets 1
>   including agent-circuit-id and agent-remote-id 1
>   preventing in L2TP ICRQ packets 1
>   relaying in L2TP tunnel-switched network 1
> Calling-Station-Id (RADIUS attribute 31) 1
>   including IOA number in format 1
> captive portal. 1, See guided entrance
> Change-of-Authorization-Request messages 1
> Cisco NAS Port Info AVP 1
>   relaying in L2TP tunnel-switched network 1
> Class (RADIUS attribute 25) 1
> clear ip commands 1
>   clear ip dhcp-local binding 1
>   clear ip routes download 1
> CLI (command-line interface) 1
>   authorization and authentication messages 1
>   commands used to modifyRADIUS attributes 1
> client-name command 1
> CoA-Request messages 1
>   guided entrance 1
>   Service Manager 1
> combined IPv4 and IPv6 services 1
>   example 1
>     with input traffic flow 1
>     with output traffic flow 1
>   example scenario 1
>     for rate limiting VoIP traffic 1
>   external parent groups and 1
>     example 1
>   in a dual stack 1
>     activating 1
>     backward compatibility 1
>     deactivating 1
>     example 1
>     performance impact 1
>   rate limiting and 1
>     example 1
>   service interim accounting 1
>   statistics collection and 1
>     external parent groups 1
> command-line interface. 1, See CLI
> Common Open Policy Service. 1, See COPS
> compatibility with previous releases 1
>   for IPv4 and IPv6 services 1
>     in a dual stack, combined 1
>     in a dual stack, independent 1
> configuring. 1, See specific feature, product, or protocol
> Connect-Info (RADIUS attribute 77) 1
> conventions 1
>   notice icons 1
>   text and syntax 1
> COPS (Common Open Policy Service) 1
> COPS(Common Open Policy Service) 1
> COPS-PR (COPS usage for policy provisioning) 1
> customer support 1
>   contacting JTAC 1

D

> Deactivate-Service (RADIUS attribute 26-66) 1
> deadtime command 1
> default domain name 1
> default-router command 1
> default-upper-type mlppp command 1
> delegating routers 1
>   allocation of IPv6 prefixes 1
>     to requesting routers 1
>   as E-Series routers 1
>     for allocation of prefixes 1
>   assigning prefixes 1
>     to DHCPv6 clients 1
> deny command 1
> descriptive formats 1
>   Calling Number AVP 1
> destination 1
>   changing 1
> DHCP (Dynamic Host Configuration Protocol) 1
>   access model 1
>   configuring BOOTP Relay 1
>   configuring DHCP relay 1
>   configuring DHCP relay proxy 1
>   configuring proxy client and server 1
>   features 1
>   giaddr 1
>   option 82 1
>   overview 1
>   per-interface logging 1
>   source IP address 1
>   trust-all 1
> DHCP access model 1
>   configuring 1
> DHCP broadcast flag 1
>   interaction with layer 2 unicast transmission method 1
> DHCP client bindings 1
>   deleting 1
>   managing 1
>   viewing 1
> DHCP commands 1
>   dhcp-external duplicate-mac-address 1
>   ip auto-detect ip-subscriber 1
>   ip dhcp-capture 1
>   ip dhcp-external re-authenticate-subscriber-interface 1
>   ip dhcp-external recreate-subscriber-interface 1
>   ip inactivity-timer 1
>   set ip interface-profile 1
>   set ip source-prefix 1
>   show dhcp-external 1
>   See also
> dhcp delete-binding command 1
> DHCP external server 1
>   and DHCP relay proxy 1
>   configuring 1
>   dynamic subscriber interfaces 1
>     interoperating with DHCP relay and DHCP relay proxy 1
>   identifying clients with duplicate MAC addresses 1
>   monitoring 1
>   preserving dynamic subscriber interfaces 1
>   re-authenticating auto-detected dynamic subscriber interfaces 1
> DHCP local address pools 1
>   configuring 1
>   grace periods 1
>   linking 1
> DHCP local server 1
>   configuring 1
>   configuring authentication 1
>   duplicate clients 1
>   equal-access mode 1
>     address allocation 1
>     configuring 1
>     connection process 1
>     local pool selection 1
>     overview 1
>     SRC (Session and Resource Control software) 1
>   local address pool group 1
>   local pool selection, equal-access 1
>     using domain name 1
>     using framed IP address 1
>     using giaddr 1
>     using pool name 1
>   local pool selection, standalone 1
>     using giaddr 1
>     using received interface IP address 1
>   logging information 1
>   modes 1
>   monitoring 1
>   overview 1
>   RADIUS accounting support for 1
>   standalone mode 1
>     address allocation 1
>     authentication 1
>     configuring 1
>     local pool selection 1
>     overview 1
>   unique client IDs 1
> DHCP local server traps 1
>   logging 1
> DHCP logging 1
> DHCP option 60 cable modem DHCP relay 1
> DHCP option 60 strings 1
> DHCP options and RADIUS 1
>   configuring 1
> DHCP packets 1
>   logging 1
> DHCP per-interface information 1
>   logging 1
> DHCP pool commands 1
>   default-router 1
>   dns-server 1
>   domain-name 1
>   grace-period 1
>   ip dhcp-local pool 1
>   lease 1
>   link 1
>   netbios-name-server 1
>   netbios-node-type 1
>   network 1
>   reserve 1
>   server-address 1
>   snmpTrap 1
>   use-release-grace-period 1
>   warning 1
> DHCP proxy client 1
>   configuring 1
> DHCP relay 1
>   configuring 1
>   creating 1
>   in same VR as dynamic subscriber interfaces 1
>   interoperating with DHCP external server 1
>   logging information 1
>   preventing host route installation 1
>   removing 1
>   spoofed giaddr 1
>   spoofed relay agent option 1
> DHCP relay agent information option 1
>   agent circuit ID (suboption 1) 1
>   agent remote ID (suboption 2) 1
>   vendor-specific (suboption 9) 1
> DHCP relay and BOOTP relay 1
>   configuring 1
> DHCP relay proxy 1
>   best offer 1
>   configuring 1
>   first offer 1
>   interoperating with DHCP external server 1
> DHCP server 1
>   dynamic subscriber interfaces 1
> DHCP vendor class identifier option 1
> dhcp-external commands 1
>   dhcp-external duplicate-mac-address 1
>   show dhcp-external 1
> DHCP-GI-Address (RADIUS attribute 26-57) 1
> dhcp-local-server-configuration-overview 1
> DHCP-MAC-Address (RADIUS attribute 26-56) 1
> DHCP-Options (RADIUS attribute 26-55) 1
> DHCPv6 clients 1
>   assigning prefixes to 1
>     using local address pools 1
> DHCPv6 local address pools 1, See IPv6 local address pools
> DHCPv6 local server 1
>   IPv6 1
> DHCPv6 Prefix Delegation 1
>   and IPv6 Neighbor Discovery 1
>     without configuring Delegated-IPv6-Prefix 1
>   assigned prefix length of /128 1
>     in local address pools 1
>   enabling 1
>     IPv6 local address pool feature 1
>   example for non-PPP client requests 1
>   example scenario 1
>   for client requests 1
>     over non-PPP links 1
>     over PPP links 1
>   for IPv6 clients 1
>     overview 1
>   Framed-IPv6-Prefix 1
>     in Access-Accept messages 1
>   guidelines for configuring 1
>     IPv6 local address pools 1
>   interface level configuration 1
>     versus router level configuration 1
>   IPv6 local address pool 1
>     mapping to a domain name 1
>   limitation on 1
>     prefixes assigned to clients 1
>   standard RADIUS attributes 1
>     configuring 1
>     verifying 1
>   using IPv6 local address pools 1
>     monitoring a single pool 1
>     monitoring all configured pools 1
>     monitoring statistics for a pool 1
> dialed number identification service. 1, See DNIS
> digital subscriber line access multiplexers. 1, See DSLAMs
> digital subscriber lines. 1, See DSLs
> disable proxy lcp command 1
> Disconnect-Cause (RADIUS attribute 26-51) 1
> Disconnect-Request messages 1
> DNIS (dialed number identification service) 1
> DNS (Domain Name System) 1
>   assigning IP addresses 1
>   overview 1
> DNS addresses 1
>   order of preference 1
>     in allocation to clients 1
> DNS domain names 1
>   list of 1
>     configured in IPv6 local address pools 1
>   order of preference 1
>     in responses to clients 1
> DNS domains 1
>   configuring more than one 1
>     using the CLI interface 1
>   in IPv6 local address pools 1
>     processing client requests for resolution 1
>   in responses to clients 1
>     Domain Search List option and 1
>   maximum number 1
>     in IPv6 local address pools 1
> DNS Recursive Name Search option 1
>   DHCPv6 server responses 1
>     and DNS servers in local pools 1
> DNS servers 1
>   addresses in responses to clients 1
>     DNS Recursive Name Search option and 1
>   configuring in 1
>     IPv6 local address pools 1
>   list of 1
>     configured in IPv6 address pools 1
>   order of preference 1
>     in responses to clients 1
>   order of use 1
>     for delegating prefixes 1
>   primary and secondary 1
>     for domain resolution requests from clients 1
>   responding with IPv6 addresses 1
>     for client requests 1
> documentation set 1
>   comments on 1
> domain command 1
> Domain Name System. 1, See DNS
> domain names 1
>   allowing or denying 1
>   configuring 1
>   default 1
>   mapping to virtual routers 1
>   mapping user requests without domain name 1
>   none 1
>   specifying single name for users 1
>   stripping domain name 1
>   using aliases 1
>   using delimiters other than @ 1
>   using either domain or realm asdomain name 1
>   using realm name as domain name 1
> Downstream-Calculated-QoS-Rate (RADIUS attribute 26-141) 1
> DSL Forum VSAs 1
>   controlling inclusion of 1
>   descriptions 1
>   in AAA access and accounting messages 1
> DSLAMs (digital subscriber line access multiplexers) 1
> DSLs (digital subscriber lines) 1
> dual stack 1
>   combined IPv4 and IPv6 services 1
>     example of 1
>   IPv4 and IPv6 services 1
>     combined, activating and deactivating 1
>     combined, overview 1
>     independent, activating and deactivating 1
>     independent, overview 1
>     service interim accounting, overview 1
>     Service manager support, activating and deactivating 1
>     Service manager support, overview 1
>   statistics collection 1
>     external parent groups 1
> duplicate AAA accounting 1
>   configuring 1
> duplicate clients 1
> duplicate MAC addresses 1
>   identifying DHCP clients with 1
>   monitoring 1
> Dynamic Host Configuration Protocol. 1, See DHCP
> dynamic IP interfaces 1
> dynamic subscriber interfaces 1
>   commands 1
>   configuring 1
>   configuring DHCP external server to interoperate with DHCP relay and DHCP relay proxy 1
>   configuring DHCP external server to preserve 1
>   configuring DHCP external server to re-authenticate 1
>   DHCP server 1
>   framed routes 1
>   GRE tunnel configuration 1
>   in same VR as DHCP relay 1
>   inheriting MAC validation state 1
>   IP over bridged Ethernet configuration 1
>   IP over Ethernet configuration 1
>   IP over VLAN over Ethernet configuration 1
>   monitoring 1
>   overview 1
>   packet detection 1

E

> E120 and E320 routers 1
>   ATM interfaces 1
> EAP (Extensible Authentication Protocol) 1
>   external RADIUS server 1
>   local authentication server 1
>   RADIUS attributes 1
>   RADIUS authentication 1
>   TACACS+ server 1
> EAP-Message (RADIUS attribute 79) 1
> Egress-Policy-Name (RADIUS attribute 26-11) 1
> enable proxy authenticate command 1
> encapsulation commands 1
>   encapsulation bridge1483 1
>   encapsulation vlan 1
> endpoint discriminator 1
> equal-access DHCP local server 1
> Ethernet 1
>   configuring dynamic subscriber interfaces 1
> Ethernet interfaces 1
>   commands 1
>     interface tenGigabitEthernet 1
> Ethernet links 1
>   between CPE and PE routers 1
>     pool section for Prefix Delegation 1
> Event-Timestamp (RADIUS attribute 55) 1
> exclusion ranges 1
>   configuring 1
>     for delegation of prefixes 1
>   example for non-PPP client requests 1
>   for DHCPv6 prefixes 1
>     delegated to clients 1
> Extensible Authentication Protocol. 1, See EAP
> external parent groups 1
>   combined IPv4 and IPv6 services with 1
>     example 1
>   statistics collection for 1
>     setting up 1

F

> fixed format 1
>   Calling Number AVP 1
> fragmentation 1
>   and reassembly 1
>   packet 1
> framed routes dynamic subscriber interfaces 1
> Framed-Compression (RADIUS attribute 13) 1
> Framed-Interface-Id (RADIUS attribute 96) 1
> Framed-Ip-Address (RADIUS attribute 8) 1
> Framed-Ip-Netmask (RADIUS attribute 9) 1
> Framed-Ipv6-Prefix (RADIUS attribute 97) 1
> Framed-IPv6-Prefix attribute 1
>   used for DHCPv6 Prefix Delegation 1
>     from Access-Accept messages 1
> Framed-MTU (RADIUS attribute 12) 1

G

> giaddr 1
> GRE (Generic Routing Encapsulation) tunnels dynamic subscriber interfaces 1
> guided entrance 1
>   CoA-Request messages 1

H

> HTTP local server 1
>   guided entrance service 1
>   Service Manager 1

I

> I/O adapters. 1, See IOAs
> identification command 1
> idle timeout for B-RAS 1
>   configuring 1
> idle timeout, range for 1
> include commands 1
>   include circuit-id 1
>   include dhcp-option 82 1
>   include hostname 1
>   include ip-address 1
>   include mac-address 1
>   include virtual-router-name 1
> independent IPv4 and IPv6 services 1
>   in a dual stack 1
>     activating 1
>     backward compatibility 1
>     deactivating 1
>     performance impact 1
>   service interim accounting 1
>   statistics collection and 1
>     external parent groups 1
> Ingress-Policy-Name (RADIUS attribute 26-10) 1
> inheriting MAC address validation state 1
> interface commands 1
>   interface atm 1
>   interface fastEthernet 1
>   interface gigabitEthernet 1
>   interface ip 1
>   interface loopback 1
>   interface tenGigabitEthernet 1
> Interface-Desc (RADIUS attribute 26-63) 1
> interfaces 1
>   configuring for DHCP local server 1
>   moving 1
> Interim-Acct messages 1
>   ANCP (L2C)-related VSAs 1
>   DSL Forum VSAs 1
> Internet Protocol. 1, See IP
> IOAs 1
>   including in RADIUS Calling-Station-Id format 1
> IP 1
>   hinting 1
> IP addresses 1
>   assigning to name servers 1
>   configuring for remote client 1
> ip commands 1
>   clear ip demux 1
>   ip address 1
>   ip address-pool dhcp 1
>   ip auto-configure ip-subscriber 1
>   ip auto-detect ip-subscriber 1
>   ip demux-type 1
>   ip destination-prefix 1
>   ip dhcp-local pool 1
>   ip inactivity-timer 1
>   ip local alias 1
>   ip local pool 1
>   ip local pool snmpTrap 1
>   ip local pool warning 1
>   ip local shared-pool 1
>   ip route-map ip-subscriber 1
>   ip service-profile 1
>   ip share-interface 1
>   ip share-nexthop 1
>   ip source-prefix 1
>   ip unnumbered 1
>   ip use-framed-routes ip-subscriber 1
>   ip-hint 1
> ip dhcp-external commands 1
>   ip dhcp-external auto-configure 1
>   ip dhcp-external disregard-giaddr-next-hop 1
>   ip dhcp-external recreate-subscriber-interface 1
>   ip dhcp-external server-address 1
>   ip dhcp-external server-sync 1
>   ip re-authenticate-auto-detect ip-subscriber 1
>   See also
> ip dhcp-local auth domain command 1
> ip dhcp-local auth include command 1
> ip dhcp-local auth password 1
> ip dhcp-local auth user-prefix command 1
> ip dhcp-local commands 1
>   ip dhcp-local auto-configure agent-circuit-identifier 1
>   ip dhcp-local excluded-address 1
>   ip dhcp-local limit 1
>   ip dhcp-local pool 1
>   ip dhcp-local unique-client-ids 1
> ip dhcp-server commands 1
>   ip dhcp-server 1
> ip http commands 1
>   ip http 1
>   ip http access-class 1
>   ip http max-connection-time 1
>   ip http port 1
>   ip http redirecturl 1
>   ip http same-host-limit 1
>   ip http server 1
> IP interfaces 1
>   creating 1
> IP interfaces that support PPP clients 1
>   configuring 1
> IP spoofing 1
>   preventing 1
> IPv4 and IPv6 services 1
>   combined services in a dual stack 1
>     example 1
>   in a dual stack 1
>     and Service Manager support 1
>   See also See also
> IPv4 services 1
>   in a dual stack 1
>     activating 1
>     combined and independent configuration 1
>     deactivating 1
>     with IPv6 services 1
> ipv6 commands 1
>   ipv6 virtual-router 1
>   ipv6-local-interface 1
>   ipv6–prefix-pool-name 1
> IPv6 DHCP local server 1
>   monitoring 1
> ipv6 dhcpv6-local commands 1
>   ipv6 dhcpv6-local delegated-prefix 1
>   ipv6 dhcpv6-local dns-domain-search 1
>   ipv6 dhcpv6-local dns-server 1
>   ipv6 dhcpv6-local prefix-lifetime 1
> IPv6 local address pools 1
>   and overriding using the RADIUS attribute from AAA server 1
>   assigned prefix length of /128 1
>     Prefix Delegation and 1
>   configuring 1
>     for Prefix Delegation 1
>   DNS servers in 1
>     to return to clients 1
>   enabling 1
>   example for non-PPP client requests 1
>   for delegation of prefixes 1
>     overview 1
>   for DHCPv6 Prefix Delegation 1
>     single pool details, viewing 1
>     statistics for a single pool, viewing 1
>     summary of all configured pools, viewing 1
>   guidelines for configuration 1
>   limitation on 1
>     number of allocated prefixes 1
>   mapping to a domain name 1
>     for Prefix Delegation 1
>   multiple configuration 1
>     on virtual router, preference order 1
>   name length 1
>   not configured in domain map 1
>     method for determining prefix to be delegated 1
>   order of preference 1
>     in selection for delegation of prefixes 1
>   Prefix Delegation 1
>     example scenario 1
>   prerequisite for configuring 1
>   procedure 1
>     for configuring on a virtual router 1
>   removing from 1
>     domain map 1
>   specifying 1
>     domain name for DNS resolution 1
>     exclusion range for prefixes 1
>     IPv6 address of DNS server 1
>     preferred lifetime 1
>     prefix range 1
>     starting and ending prefixes of a range 1
>     valid lifetime 1
>   used for Prefix Delegation from 1
>     AAA domain map 1
>     interface address 1
>     RADIUS server 1
> IPv6 Neighbor Discovery 1
>   and DHCPv6 Prefix Delegation 1
>     without configuring Delegated-IPv6-Prefix 1
>   IPv6-NdRa-Prefix 1
>     in Access-Accept messages 1
>   standard RADIUS attributes 1
>     configuring 1
>     verifying 1
> IPv6 prefix ranges 1
>   configuring 1
>     with the starting and ending prefixes 1
>     with the starting prefix and length 1
> IPv6 services 1
>   in a dual stack 1
>     activating 1
>     combined and independent configuration 1
>     deactivating 1
>     with IPv4 services 1
> IPv6-NdRa-Prefix attribute 1
>   used for IPv6 Neighbor Discovery 1
>     from Access-Accept messages 1

K

> key command 1

L

> L2C-Down-Stream-Data (RADIUS attribute 26-93) 1
> L2C-Information (RADIUS attribute 26-81) 1
> L2C-Up-Stream-Data (RADIUS attribute 26-92) 1
> L2TP (Layer 2 Tunneling Protocol) 1
>   defining 1
>   high availability considerations 1
>   implementation 1
>   license 1
>   modifying LAC default settings 1
>   monitoring 1
>   peer resynchronization 1
>   rx speed 1
>   sessions supported 1
>   silent failover 1
>   tunnel selection 1
>   tunnel switch profiles 1
> L2TP access concentrator. 1, See LAC
> l2tp commands 1
>   disconnect-cause 1
>   failover-resync 1
>   l2tp checksum 1
>   l2tp destination lockout-test 1
>   l2tp destination lockout-timeout 1
>   l2tp destination profile 1
>   l2tp destruct-timeout 1
>   l2tp disable calling-number avp 1
>   l2tp disable challenge 1
>   l2tp disconnect-cause 1
>   l2tp drain 1
>   l2tp drain destination 1
>   l2tp drain tunnel 1
>   l2tp fail-over-within-preference 1
>   l2tp failover-resync 1
>   l2tp ignore-receive-data-sequencing 1
>   l2tp ignore-transmit-address-change 1
>   l2tp reject-transmit-address-change 1
>   l2tp retransmission 1
>   l2tp short-drain-timeout 1
>   l2tp shutdown 1
>   l2tp shutdown destination 1
>   l2tp shutdown session 1
>   l2tp shutdown tunnel 1
>   l2tp switch-profile 1
>   l2tp tunnel default-receive-window 1
>   l2tp tunnel idle-timeout 1
>   l2tp tunnel test 1
>   l2tp tunnel-switching 1
>   l2tp unlock destination 1
>   l2tp unlock-test destination 1
>   l2tp weighted-load-balancing command 1
>   max-sessions command 1
>   See also
> L2TP dial-out 1
>   before configuring 1
>   configuring 1
>   dial-out process 1
>   network model 1
>   operational states 1
>   outgoing call setup details 1
>     Access-Accept message 1
>     Access-Request message 1
>     mutual authentication 1
>     outgoing call successful 1
>     route installation 1
>   overview 1
>   references 1
>   route 1
>   session 1
>   target 1
>   trigger 1
> l2tp dial-out commands 1
>   l2tp dial-out connecting-timer-value 1
>   l2tp dial-out dormant-timer-value 1
>   l2tp dial-out max-buffered-triggers 1
>   l2tp dial-out session delete 1
>   l2tp dial-out session reset 1
>   l2tp dial-out target 1
>   See also
> L2TP network server. 1, See LNS
> L2TP RWS (receive window size) 1
>   configuring global default 1
>   configuring on LAC 1
>   configuring on LNS 1
>   l2tp tunnel default-receive-window command 1
>   overview 1
>   receive-window command (for LAC) 1
>   receive-window command (for LNS) 1
>   show l2tp command 1
>   show l2tp destination profile command 1
> l2tp rx-connect-speed-when-equal command 1
> L2TP transmit connect speed 1
>   and Transmit (TX) Speed AVP 24 1
>   calculation methods 1
>     how to configure 1
>   monitoring 1
> L2TP transmit connect speed and Transmit (TX) Speed AVP 24 1
>   calculation methods 1
>     actual 1
>     dynamic layer 2 1
>     examples 1
>     QoS 1
>     static layer 2 1
>   configuring 1
>     AAA default tunnel parameters 1
>     AAA domain maps 1
>     AAA tunnel groups 1
>     RADIUS 1
>   reporting considerations 1
> L2TP tunnel switch profiles 1
>   applying default profile 1
>   applying through AAA domain maps 1
>   applying through AAA tunnel groups 1
>   applying through RADIUS 1
>   AVP relay, configuring 1
>   configuration guidelines 1
>   configuring 1
>   how to apply 1
>   monitoring 1
> LAC (L2TP access concentrator) 1
>   before configuring 1
>   configuring receive window size (RWS) 1
>   function 1
>   sequence of events 1
> Layer 2 Tunneling Protocol. 1, See L2TP
> license commands 1
>   license b-ras 1
>   license l2tp-session 1
>   license service-manager 1
>   See also
> licenses 1
>   B-RAS 1
>   L2TP 1
>   Service Manager 1
> lifetime 1
>   guideline 1
>     for preferred lifetime 1
>   preferred 1
>     configuring for Prefix Delegation 1
>   restriction 1
>     in configuration for delegated prefixes 1
>   specifying 1
>     as infinite 1
>   valid 1
>     configuring for Prefix Delegation 1
> limitation 1
>   on number of IPv6 prefixes 1
>     delegated to clients 1
> line command 1
> LLID (logical line identifier) 1
>   configuration steps 1
>   how it works 1
>   monitoring 1
>   preauthentication considerations 1
>   RADIUS attributes in preauthentication request 1
>   troubleshooting 1
>   using to track subscribers 1
> LNS (L2TP network server) 1
>   before configuring 1
>   configuring 1
>   configuring receive window size (RWS) 1
>   installing multiple tunnel-service modules 1
>   modules supported 1
>   out-of-resource result codes 1
>   overriding out-of-resource result codes 1
>   sequence of events 1
> local address pool 1
>   alias names 1
>   mapping to domain name 1
>   ranges 1
> local address server 1
>   alias names 1
>   configuring 1
>   pool ranges 1
>   shared local address pools 1
>   SNMP thresholds 1
> local authentication commands 1
>   aaa authentication default 1
>   aaa local database 1
>   aaa local select database 1
>   aaa local username 1
>   ip-address 1
>   ip-address-pool 1
>   operational-virtual-router 1
>   password 1
>   secret 1
>   username 1
> local host command 1
> local ip address command 1
> local-interface command 1
> logging. 1, See specific feature, product, or protocol
> logical line identifier, AAA. 1, See LLID
> login authentication command 1
> logout subscribers command 1

M

> MAC (media access control) addresses 1
>   duplicate 1
>   inheriting validation state 1
>   preventing IP spoofing 1
> macros 1
>   service definitions 1
>   Service Manager statistics 1
> manuals 1
>   comments on 1
> max-sessions command 1
> MBS (RADIUS attribute 26-17) 1
> media access control addresses. 1, See MAC addresses
> medium ipv4 command 1
> merging policies 1
>   naming conventions 1
> Message-Authenticator (RADIUS attribute 80) 1
> MLPPP Bundle Name (RADIUS attribute 26-62) 1
> monitoring. 1, See specific feature, product, or protocol
> mutex service 1

N

> name server addresses 1
>   configuring 1
> naming conventions 1
>   merged policies 1
> NAS (network access server) 1
> NAS-Identifier (RADIUS attribute 32) 1
> NAS-IP-Address (RADIUS attribute 4) 1
> NAS-Port (RADIUS attribute 5) 1
> NAS-Port-Id (RADIUS attribute 87) 1
> NAS-Port-Type (RADIUS attribute 61) 1
> nas-port-type atm command 1
> NAS-Port-Type attribute, manually setting 1
> nas-port-type ethernet command 1
> network access server. 1, See NAS
> network commands 1
>   network 1
> no radius client command 1
> non-PPP clients 1
>   pool section for Prefix Delegation 1
> non-PPP equal access 1
>   configuration example 1
>   requirements 1
> none domain name 1
> notice icons 1

O

> operational states, L2TP 1
>   chassis 1
>   sessions 1
>   targets 1
>   virtual router 1
> option 82 1
> out-of-resource result codes, LNS 1
> Output-Gigawords (RADIUS attribute 53) 1
> override-user command 1

P

> packet detection dynamic subscriber interfaces 1
> packet fragmentation 1
> packet mirroring 1
> packets 1
>   demultiplexing 1
>   transmitting 1
> password command 1
> PCR (RADIUS attribute 26-15) 1
> peer 1
> peer resynchronization 1
> performance impact 1
>   IPv4 and IPv6 services 1
>     in a dual stack, combined 1
>     in a dual stack, independent 1
> persistent tunnels, creating 1
> PIB (Policy Information Base) 1
> platform considerations 1
>   PPP 1
> Point-to-Point Protocol. 1, See PPP
> Policy Information Base. 1, See PIB
> policy management on subscriber interfaces 1
> PPP (Point-to-Point Protocol) 1
>   accounting statistics for tunneled sessions 1
>   B-RAS service support 1
>   platform considerations 1
> ppp commands 1
>   ppp aaa-profile 1
> PPPoE remote circuit ID 1
> Pppoe-Description (RADIUS attribute 26-24) 1
> pre-authenticate command 1
> preauthentication 1
>   AAA LLID 1
>   B-RAS users 1
> preference 1
> preference command 1
> preference order 1
>   in allocation of prefixes 1
>     to IPv6 clients 1
>   in assignment of DNS addresses 1
>     to IPv6 clients 1
>   in determining local address pool 1
>     for allocation of IPv6 prefixes 1
> preferred lifetime 1
>   for delegated prefixes 1
>     configuring 1
>     default 1
>   setting 1
>     without expiration 1
> Prefix Delegation 1, See DHCPv6 Prefix Delegation
> prefixes 1
>   allocated to clients from 1
>     interface configuration 1
>     IPv6 local address pools 1
>     RADIUS Access-Accept message 1
>   assigned length of /128 1
>     in IPv6 local address pools 1
>   assigning to 1
>     DHCPv6 clients 1
>   configuring ranges 1
>     for delegation to clients 1
>   delegating by 1
>     DHCPv6 local server 1
>   delegating to clients 1
>     over non-PPP links 1
>     over PPP links 1
>   excluded from 1
>     delegation to clients 1
>   excluding 1
>     range and individual ones 1
>   in Access-Accept messages 1
>     applicable RADIUS attributes 1
>     for DHCPv6 Prefix Delegation 1
>     priority over prefix in local address pool 1
>   limitation on 1
>     number assigned to clients 1
>   order of preference 1
>     in allocation to clients 1
>   preferred and valid lifetimes 1
>     configuring for delegated ones 1
> prerequisite 1
>   for configuring IPv6 local address pools 1
>     for Prefix Delegation 1
> primary authentication/accounting RADIUS server 1
> primary IP interface 1
> privilege authentication, TACACS+ 1
> profile commands 1
>   profile 1

Q

> QoS (quality of service) 1
>   calculation method for L2TP transmit connect speed 1
>   on subscriber interfaces 1
> QoS commands 1
>   qos-parameter 1
>   qos-profile 1

R

> RADIUS (Remote Authentication Dial-In User Service) 1
>   AAA failure 1
>   accounting methods 1
>   attribute descriptions 1
>   attributes supported 1
>   authentication and accounting servers 1
>   authentication methods 1
>   Calling-Station-Id formats supported 1
>   change of authority messages 1
>   CLI AAA messages 1
>   client to server interaction 1
>   configuring servers 1
>   description 1
>   direct server access 1
>   disconnect messages 1
>   EAP authentication 1
>   IETF attributes supported 1
>   Juniper Networks VSAs supported 1
>   L2TP transmit connect speed 1
>   L2TP tunnel switch profiles, applying 1
>   message types supported 1
>   RADIUS dynamic-request server 1
>   round-robin server access 1
>   server access 1
>   server request processing limit 1
>   Service Manager attributes 1
>   Service Manager tags 1
>   services 1
>   SNMP traps 1
>   system log messages 1
>   traffic shaping for PPP over ATM interfaces 1
>   VSAs (vendor-specific attributes) 1
>     for dynamic IP interfaces 1
>     formats 1
> RADIUS attributes 1
>   preference order and 1
>     allocation of prefixes to IPv6 clients 1
> radius commands 1
>   radius acct-session-id-format 1
>   radius algorithm 1
>   radius calling-station-delimiter 1
>   radius calling-station-format 1
>   radius client 1
>   radius connect-info-format 1
>   radius connect-info-format command 1
>   radius disconnect client 1
>   radius dsl-port-type 1
>   radius dynamic-request server 1
>   radius ethernet-port-type 1
>   radius ignore atm-mbs 1
>   radius ignore atm-pcr 1
>   radius ignore atm-scr 1
>   radius ignore atm-service-category 1
>   radius ignore egress-policy-name 1
>   radius ignore framed-ip-netmask 1
>   radius ignore ingress-policy-name 1
>   radius ignore virtual-router 1
>   radius include 1
>     ANCP (L2C)-related Juniper Networks VSAs 1
>   radius include access-loop-parameters 1
>   radius include acct-authentic 1
>   radius include acct-delay-time 1
>   radius include acct-link-count 1
>   radius include acct-multi-session-id 1
>   radius include acct-session-id 1
>   radius include acct-session-id access-request 1
>   radius include acct-terminate-cause 1
>   radius include acct-tunnel-connection 1
>   radius include ascend-num-in-multilink 1
>   radius include called-station-id 1
>   radius include calling-station-id 1
>   radius include class 1
>   radius include connect-info 1
>   radius include dhcp-gi-address 1
>   radius include dhcp-mac-address 1
>   radius include dhcp-options 1
>   radius include downstream-calculated-qos-rate 1
>   radius include dsl-forum-attributes 1
>   radius include egress-policy-name 1
>   radius include event-timestamp 1
>   radius include framed-compression 1
>   radius include framed-interface-id 1
>   radius include framed-ip-add acct-start 1
>   radius include framed-ip-addr 1
>   radius include framed-ip-netmask 1
>   radius include framed-ipv6-prefix 1
>   radius include ingress-policy-name 1
>   radius include input-gigapkts 1
>   radius include input-gigawords 1
>   radius include interface-description 1
>   radius include l2c-downstream-data 1
>   radius include l2c-upstream-data 1
>   radius include l2tp-ppp-disconnect-cause 1
>   radius include mlppp-bundle-name 1
>   radius include nas-identifier 1
>   radius include nas-port 1
>   radius include nas-port-id 1
>   radius include nas-port-type 1
>   radius include output-gigapkts 1
>   radius include output-gigawords 1
>   radius include pppoe-description 1
>   radius include profile-service-description 1
>   radius include tunnel-assignment-id 1
>   radius include tunnel-client-auth-id 1
>   radius include tunnel-client-endpoint 1
>   radius include tunnel-interface-id 1
>   radius include tunnel-medium-type 1
>   radius include tunnel-preference 1
>   radius include tunnel-server-attributes 1
>   radius include tunnel-server-auth-id 1
>   radius include tunnel-server-endpoint 1
>   radius include tunnel-type 1
>   radius include upstream-calculated-qos-rate 1
>   radius includeframed-ip-netmask 1
>   radius nas-identifier 1
>   radius nas-port-format 1
>   radius nas-port-format extended atm 1
>   radius nas-port-format extended ethernet 1
>   radius override calling-station-id remote-circuit-id 1
>   radius override nas-info 1
>   radius override nas-ip-addr tunnel-client-endpoint 1
>   radius override nas-port-id remote-circuit-id 1
>   radius pppoe nas-port-format unique 1
>   radius pre-authentication server 1
>   radius relay server 1
>   radius relay udp-checksum 1
>   radius remote-circuit-id-delimiter 1
>   radius remote-circuit-id-format 1
>   radius rollover-on-reject 1
>   radius route-download server 1
>   radius server 1
>   radius trap acct-server-not-responding 1
>   radius trap acct-server-responding 1
>   radius trap auth-server-not-responding 1
>   radius trap auth-server-responding 1
>   radius trap no-acct-server-responding 1
>   radius trap no-auth-server-responding 1
>   radius tunnel-accounting 1
>   radius udp-checksum 1
>   radius update-source-addr 1
>   radius vlan nas-port-format stacked 1
>   See also
> RADIUS dynamic-request server 1
>   change of authorization messages 1
>   disconnect messages 1
>   how it works 1
>   message exchange 1
>   monitoring 1
>   overview 1
>   qualifications for disconnect 1
>   security and authentication 1
>   Service Manager 1
> RADIUS IPv6 attributes 1
>   configuring 1
>     for DHCPv6 Prefix Delegation 1
>     for IPv6 Neighbor Discovery 1
>   verifying 1
>     for DHCPv6 Prefix Delegation 1
>     for IPv6 Neighbor Discovery 1
> RADIUS relay server 1
>   configuring 1
>   monitoring 1
> radius remote-circuit-id-format command 1
> RADIUS route-download server 1
>   configuring 1
>   format of routes 1
>   how it works 1
>   per chassis 1
>   supported attributes 1
> RADIUS servers 1
>   attributes in Access-Accept 1
>     overriding configured local pool 1
>   attributes used for 1
>     DHCPv6 Prefix Delegation 1
>   Prefix Delegation and 1
>     pool name not returned in Access-Accept 1
>     pool name returned in Access-Accept 1
> radius-attributes-override-monitoring 1
> RADIUS-initiated change of authorization 1
>   qualifications for change of authorization 1
> RADIUS-initiated disconnect 1
>   configuring 1
>   L2TP LAC users 1
>   references 1
>   sample network 1
>   security and authentication 1
> realm names 1
>   configuring 1
>   usage 1
> Receive speed AVP 1
> receive window size (RWS). 1, See L2TP RWS
> receive-window command 1
> redirected authentication 1
> remote access (B-RAS). 1, See B-RAS applications
> Remote Authentication Dial-In User Service. 1, See RADIUS
> remote clients, IP addresses for 1
> remote host command 1
> remote system 1
> requesting routers 1
>   as customer edge device 1
>     in obtaining IPv6 prefixes 1
>   assigning prefixes to 1
>     using IPv6 local address pools 1
>   receipt of IPv6 prefixes 1
>     from delegting routers 1
> retransmit command 1
> router-name command 1
> RX speed AVP 1

S

> S-VLAN links 1
>   between CPE and PE routers 1
>     pool section for Prefix Delegation 1
> SCR (RADIUS attribute 26-16) 1
> SDX (Service Deployment System) software 1
>   See also
> server-name command 1
> service commands 1
>   service dhcp-external 1
>   service dhcp-local 1
>   service dhcp-local authenticate 1
>   service dhcpv6-local 1
>   service-description 1
> service definitions 1
>   copying 1
>   creating 1
>   installing 1
>   modifying 1
>   modifying QoS configurations 1
>   specifying parameter instances 1
>   specifying QoS profiles 1
>   uninstalling 1
> service instance 1
> service interim accounting 1
>   in a dual stack 1
>     of IPv4 and IPv6 services 1
>   IPv4 and IPv6 services 1
>     overview 1
> Service Manager 1
>   CLI support 1
>   CoA-Request messages 1
>   combined IP4 and IPv6 service 1
>     example 1
>   configuring 1
>     Service Manager license 1
>   deactivating 1
>     setting thresholds 1
>   guided entrance 1
>   IPv4 and IPv6 services 1
>     combined, activating 1
>     combined, deactivating 1
>     combined, overview 1
>     in a dual stack, activating 1
>     in a dual stack, overview 1
>     independent, activating 1
>     independent, deactivating 1
>     independent, overview 1
>     overview 1
>   license sessions 1
>   macros 1
>   multiple services 1
>   mutex service 1
>   overview 1
>   parameter values 1
>   preprovisioning services 1
>   QoS 1
>     considerations 1
>     modifying configurations of 1
>     referencing configurations of 1
>     removing references of 1
>   RADIUS dynamic-request server 1
>   RADIUS support 1
>   RADIUS tags 1
>   service definition 1
>     parameters 1
>   service instance 1
>   service session 1
>     forcing deactivation 1
>     profiles 1
>   service session profiles 1
>   session thresholds 1
>   statistics 1
>     macro command 1
>     using RADIUS 1
>     using the CLI 1
>   statistics collection 1
>     for external parent groups, setting up 1
>   subscriber session ID 1
>   subscriber sessions 1
>   supported platforms 1
>   tasks 1
>   testing services 1
> Service Manager commands 1
>   no service-management owner-session force 1
>   no service-management subscriber-session force 1
>   service-management install 1
>   service-management owner-session 1
>   service-management service-session-profile 1
>   service-management subscriber-session service-session 1
>   statistics 1
>   time 1
>   volume 1
> Service Manager license 1
>   configuring 1
> service session 1
> Service-Category (RADIUS attribute 26-14) 1
> Service-Description (RADIUS attribute 26-53) 1
>   setting 1
> Service-Interim-Acct-Interval (RADIUS attribute 26-140) 1
> Service-Session (RADIUS attribute 26-83) 1
> Service-Statistics (RADIUS attribute 26-69) 1
> Service-Stats (RADIUS attribute 26-69) 1
> Service-Timeout (RADIUS attribute 26-68) 1
> Service-Volume (RADIUS attribute 26-67) 1
> session 1
> Session and Resource Control. 1, See SRC software
> session timeout 1
>   configuring 1
>   interpreting default value 1
>   range for 1
> session-out-of-resource-result-code-override command 1
> Session-Timeout (RADIUS attribute 27) 1
> sessions, L2TP 1
> set dhcp commands 1
>   set dhcp vendor-option 1
> set dhcp relay commands 1
>   set dhcp relay 1
>   set dhcp relay agent 1
>   set dhcp relay agent sub-option 1
>   set dhcp relay assign-giaddr-source-ip 1
>   set dhcp relay broadcast-flag-replies 1
>   set dhcp relay giaddr-selects-interface 1
>   set dhcp relay layer2-unicast-replies 1
>   set dhcp relay options 1
>   set dhcp relay override 1
>   set dhcp relay preserve-trusted-client-option 1
>   set dhcp relay proxy 1
>   set dhcp relay trust-all 1
> set dhcp relay proxy commands 1
>   set dhcp relay proxy 1
>   set dhcp relay proxy send-first-offer 1
>   set dhcp relay proxy timeout 1
> set dhcp vendor-option command 1
> shared IP interfaces 1
> shared local address pools 1
> shared tunnel-server ports 1
>   using with L2TP 1
> show aaa commands 1
>   show aaa accounting 1
>   show aaa accounting default 1
>   show aaa accounting interval 1
>   show aaa accounting vr-group 1
>   show aaa authentication default 1
>   show aaa delimiters 1
>   show aaa dhcpv6-delegated-prefix 1
>   show aaa domain-map 1
>   show aaa duplicate-address-check 1
>   show aaa intf-desc-format 1
>   show aaa ipv6-nd-ra-prefix 1
>   show aaa model 1
>   show aaa name-servers 1
>   show aaa profile 1
>   show aaa route-download routes 1
>   show aaa route-download routes global 1
>   show aaa service accounting interval 1
>   show aaa statistics 1
>   show aaa subscriber per-port-limit 1
>   show aaa subscriber per-vr-limit 1
>   show aaa timeout 1
>   show aaa tunnel-group 1
>   show aaa tunnel-parameters 1
>   show aaa user accounting interval 1
>   show radius route-download 1
> show configuration commands 1
>   show configuration category aaa global-attributes 1
>   show configuration category aaa local-authentication 1
>   show configuration category aaa server-attributes include-defaults 1
>   show configuration category aaaglobal-attributes 1
>   show configuration category aaalocal-authentication 1
>   show configuration category aaaserver-attributes include-defaults 1
> show cops info command 1
> show cops statistics command 1
> show dhcp commands 1
>   show dhcp binding 1
>   show dhcp count 1
>   show dhcp host 1
>   show dhcp relay 1
>   show dhcp relay proxy statistics 1
>   show dhcp relay statistics 1
>   show dhcp server 1
>   show dhcp server statistics 1
> show dhcp summary command 1
> show dhcp vendor-option command 1
> show dhcp-external command 1
> show ip commands 1
>   show ip demux interface 1
>   show ip local alias 1
>   show ip local pool 1
>   show ip local-pool statistics command 1
>   show ip service-profile 1
>   show ip-subscriber 1
> show ip dhcp-capture command 1
> show ip dhcp-external commands 1
>   show ip dhcp-external binding 1
>   show ip dhcp-external client-id 1
>   show ip dhcp-external configuration 1
>   show ip dhcp-external statistics 1
> show ip dhcp-local commands 1
>   show ip dhcp-local 1
>   show ip dhcp-local auth 1
>   show ip dhcp-local binding 1
>   show ip dhcp-local duplicate-clients 1
>   show ip dhcp-local excluded 1
>   show ip dhcp-local limits 1
>   show ip dhcp-local pool 1
>   show ip dhcp-local reserved 1
>   show ip dhcp-local statistics 1
> show ip dhcpv6-local commands 1
>   show ip dhcpv6-local binding 1
>   show ip dhcpv6-local dns-domain-searchlist 1
>   show ip dhcpv6-local dns-servers 1
>   show ip dhcpv6-local prefix-lifetime 1
>   show ip dhcpv6-local statistics 1
> show ip http commands 1
>   show ip http scalar 1
>   show ip http server 1
>   show ip http statistics 1
> show ip local shared-local command 1
> show ipv6 local pool commands 1
>   for a single pool 1
>   for all configured pools 1
>   statistics for a single pool 1
> show l2tp commands 1
>   show l2tp 1
>   show l2tp destination 1
>   show l2tp destination lockout 1
>   show l2tp destination summary 1
>   show l2tp session 1
>   show l2tp session summary 1
>   show l2tp tunnel 1
>   show l2tp tunnel summary 1
> show l2tp dial-out commands 1
>   show l2tp dial-out 1
>   show l2tp dial-out target 1
> show license commands 1
>   show license b-ras 1
>   show license service-management 1
> show profile commands 1
>   show profile 1
>   show profile name 1
> show qos commands 1
>   show qos-parameter 1
> show radius commands 1
>   show radius accounting servers 1
>   show radius accounting statistics 1
>   show radius acct-session-id-format 1
>   show radius algorithm 1
>   show radius attributes-included 1
>   show radius authentication servers 1
>   show radius authentication statistics 1
>   show radius calling-station-delimiter 1
>   show radius calling-station-format 1
>   show radius connect-info-format 1
>   show radius dsl-port-type 1
>   show radius dynamic-request servers 1
>   show radius dynamic-request statistics 1
>   show radius ethernet-port-type 1
>   show radius nas-identifier 1
>   show radius nas-port-format 1
>   show radius override 1
>   show radius pppoe nas-port-format 1
>   show radius remote-circuit-id-delimiter 1
>   show radius remote-circuit-id-format 1
>   show radius rollover-on-reject 1
>   show radius route-download statistics 1
>   show radius servers 1
>   show radius statistics 1
>   show radius trap 1
>   show radius tunnel-accounting 1
>   show radius update-source-address 1
>   show radius vlan nas-port-format 1
> show radius override 1
> show radius relay commands 1
>   show radius relay servers 1
>   show radius relay statistics 1
>   show radius relay udp-checksum 1
> show service-management commands 1
>   show service-management owner-session 1
>   show service-management service-definition 1
>   show service-management service-session-profile 1
>   show service-management subscriber-session 1
>   show service-management summary 1
> show sscc commands 1
>   show sscc info 1
>   show sscc statistics 1
>   show sscc version 1
> show subscribers command 1
> show terminate-code command 1
> SNMP traps 1
>   configuring for DHCP local servers 1
>   configuring for RADIUS servers 1
>   overview 1
> source-address command 1
> spoofing, IP 1
>   preventing 1
> SRC (Session and Resource Control) software 1
>   configuring the client 1
>   monitoring the client 1
> SRC (Session and Resource Control)software 1
> sscc commands 1
>   sscc address 1
>   sscc enable 1
>   sscc protocol ipv6 1
>   sscc retryTimer 1
>   sscc sourceAddress 1
>   sscc transportRouter 1
>   See also
> standalone DHCP local server 1
> standard RADIUS attributes 1
>   configuring 1
>     for DHCPv6 Prefix Delegation 1
>     for IPv6 Neighbor Discovery 1
>   IPv6 Neighbor Discovery and 1
>     configuring logging severity 1
>     warning message 1
>   using the same values 1
>     for Neighbor Discovery and Prefix Delegation 1
>   verifying 1
>     for DHCPv6 Prefix Delegation 1
>     for IPv6 Neighbor Discovery 1
> State (RADIUS attribute 24) 1
> statistics 1
>   for DHCPv6 Prefix Delegation 1
>     viewing 1
> statistics collection 1
>   for external parent groups 1
>     setting up 1
> strip-domain command 1
> subscriber disconnect command 1
> subscriber interface commands 1
>   set dhcp relay giaddr-selects-interface 1
> subscriber interfaces 1
>   applications 1
>   commands 1
>     configuring dynamic 1
>     configuring static 1
>   configuring 1
>     multicast routing protocols 1
>     policies and Qo 1
>     routing protocols 1
>   dynamic 1
>     inheriting MAC validation state 1
>   GRE tunnel configuration 1
>   IP over bridged Ethernet configuration 1
>   IP over Ethernet configuration 1
>   IP over VLAN over Ethernet configuration 1
>   monitoring 1
>   overview 1
>     dynamic 1
>     static 1
>   static 1
> subscribers 1
>   accounting messages 1
>   authorization and authentication messages 1
>   E-series routers 1
>   limiting active subscribers 1
>   preauthentication and AAA LLID 1
> support, technical 1, See technical support
> system log messages 1

T

> TACACS+ 1
>   AAA services 1
>   accounting 1
>   authentication login process 1
>   authorization 1
>   configuring 1
>   daemon 1
>   host 1
>   NAS (network access server) 1
>   privilege authentication 1
> TACACS+ commands 1
>   aaa accounting commands 1
>   aaa accounting exec 1
>   aaa accounting suppress null-username 1
>   aaa accounting tacacs+ 1
>   aaa authentication enable default 1
>   aaa authentication login 1
>   aaa new-model 1
>   tacas-server key 1
>   tacas-server source-address 1
>   tacas-server timeout 1
>   tacas-sever host 1
> TCP and TACACS+ 1
> technical support 1
>   contacting JTAC 1
> Terminal Access Controller Access Control System +. 1, See TACACS+
> terminate-code command 1
> test aaa command 1
> text and syntax conventions 1
> timeout command 1
> timeout, configuring for B-RAS applications 1
> traffic shaping for PPP over ATM 1
> translate command 1
> transmit connect speed, L2TP. 1, See L2TP transmit connect speed
> tunnel 1
>   defined 1
>   selection, L2TP 1
>   switching 1
> tunnel commands, L2TP 1
>   tunnel 1
>   tunnel group 1
>   tunnel password 1
> tunnel group mode, mapping to L2TP tunnel 1
> tunnel selection, L2TP 1
>   failover between preference levels 1
>   failover within preference levels 1
>   maximum sessions per tunnel 1
>   weighted load balancing 1
> tunnel subscribers, enabling authentication for 1
> tunnel switch profiles, L2TP 1
>   applying default profile 1
>   applying through AAA domain maps 1
>   applying through AAA tunnel groups 1
>   applying through RADIUS 1
>   AVP relay, configuring 1
>   configuration guidelines 1
>   configuring 1
>   how to apply 1
>   monitoring 1
> Tunnel-Assignment-Id (RADIUS attribute 82) 1
> Tunnel-Client-Auth-Id (RADIUS attribute 90) 1
> Tunnel-Client-Endpoint (RADIUS attribute 66) 1
> Tunnel-Interface-Id (RADIUS attribute 26-44) 1
> Tunnel-Medium-Type (RADIUS attribute 65) 1
> Tunnel-Preference (RADIUS attribute 83) 1
> tunnel-server command 1
> tunnel-server ports 1
>   shared 1
> Tunnel-Server-Auth-Id (RADIUS attribute 91) 1
> Tunnel-Server-Endpoint (RADIUS attribute 67) 1
> tunnel-service modules 1
>   installing multiple for LNS sessions 1
> tunnel-subscriber authentication command 1
> Tunnel-Type (RADIUS attribute 64) 1
> tunneled PPP session accounting statistics 1
> tunnels, IP 1
>   shared tunnel-server ports 1
> tx-connect-speed-method command 1
> type command, L2TP 1

U

> UDP (User Datagram Protocol) 1
>   checksums 1
> udp-port command 1
> Upstream-Calculated-QoS-Rate (RADIUS attribute 26-142) 1
> user domain, mapping to L2TP tunnel 1
> User-Name (RADIUS attribute 1) 1
> user-name command 1
> user-prefix command 1
> usernames and passwords from a domain 1
>   configuring 1
> using shared tunnel-server ports 1

V

> valid lifetime 1
>   for delegated prefixes 1
>     configuring 1
>     default 1
>   setting 1
>     without expiration 1
> validation state, inheriting for MAC addresses 1
> vendor class identifier option 1
> vendor-specific (suboption 9) 1
> vendor-specific attributes. 1, See VSAs
> virtual routers 1
>   mapping user domain names 1
>   redirected authentication 1
> Virtual-Router (RADIUS attribute 26-1) 1
> vlan commands 1
>   vlan id 1
> VLAN links 1
>   between CPE and PE routers 1
>     pool section for Prefix Delegation 1
> VLANs (virtual local area networks) 1
>   configuring dynamic subscriber interfaces 1
> VPNs (virtual private networks) 1
>   connecting subscribers 1
> VSAs (vendor-specific attributes) 1
>   DSL Forum 1
>     controlling inclusion of 1
>     descriptions 1
>     in AAA access and accounting messages 1
>   for dynamic IP interfaces 1
>   formats 1

W

> walled garden. 1, See guided entrance
> Web access to E-series router 1
> Windows Internet Name Service. 1, See WINS
> WINS, assigning IP addresses 1

[Contents] [Prev] [Next] [Index] [Report an Error]