[Contents] [Prev] [Next] [Index] [Report an Error]

# profile-reassign

#### Syntax

profile-reassign atm interfaceSpecifier { ppp | pppoe | any } profileName

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Reassigns the profile currently assigned to the specified encapsulation type for the specified ATM 1483 subinterface. For troubleshooting purposes, the profile-reassign command enables you to “ swap” the currently assigned profile for one that has PPP or PPPoE packet–logging attributes enabled. There is no no version.

| Note: Issuing the profile-reassign command causes the router to tear down any dynamic interfaces that exist above the ATM 1483 subinterface. After the profile is reassigned, the router restores the interfaces based on the necessary client reconnections.

#### Options

- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- ppp—Specifies a PPP encapsulation type to which the profile applies
- pppoe—Specifies a PPPoE encapsulation type to which the profile applies
- any—Specifies any autoconfigured encapsulation that does not have a specific profile assignment; valid only if neither the ppp encapsulation type nor the pppoe encapsulation type has an existing profile assignment
- profileName—Profile name of up to 80 characters

#### Mode

Privileged Exec (at privilege level 5 or higher)

[Contents] [Prev] [Next] [Index] [Report an Error]