[Contents] [Prev] [Next] [Index] [Report an Error]

# restricted

#### Syntax

[ no ] restricted interface restrictedInterfaceType interfaceSpecifier [ atmVpi | s-vlanIdValue ]

#### Release Information

Command introduced in JUNOSe Release 9.2.0.

#### Description

Configures an interface superset as restricted to a particular ATM-VPI or S-VLAN ID. The no version deletes the restriction for the interface superset.

#### Options

- restrictedInterfaceType—One of the following restricted interface types: atm-vp, fastEthernet, gigabitEthernet, svlan, tenGigabitEthernet
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers in About This Guide
- atmVpi—Virtual path identifier of this PVC; number in the range 0–255
- s-vlanIdValue—S-VLAN ID number in the range 0–4095

#### Mode

QoS Interface Superset Configuration

#### Related Topics

- Configuring Interface Supersets for QoS

[Contents] [Prev] [Next] [Index] [Report an Error]