[Contents] [Prev] [Next] [Index] [Report an Error]

# oam retry

#### Syntax

oam retry [ upRetryCount [ downRetryCount retryFrequency ] ]

no oam retry

#### Release Information

Command introduced in JUNOSe Release 7.1.0.
ATM VC Class Configuration mode added in JUNOSe Release 7.3.0.

#### Description

In ATM VC Configuration mode, configures parameters for F5 OAM VC integrity on an ATM PVC. The oam retry command is valid only for data PVCs; you cannot use this command for control (ILMI or signaling) PVCs. The no version restores the default values for all of these parameters.

In ATM VC Class Configuration mode, configures F5 OAM VC integrity parameters as part of a VC class definition that you assign to an ATM PVC. The no version restores the default values for all of these parameters in the VC class.

| Note: To configure the up retry count, down retry count, and retry frequency F5 OAM VC integrity parameters, you must use the oam retry command. There is no equivalent atm pvc command to configure these parameters.

#### Options

- upRetryCount—Number of successive loopback cell responses, in the range 1–60, for the router to receive before reporting that a PVC is up; default value is 3
- downRetryCount—Number of successive loopback cell responses, in the range 1–60, for the router to miss before reporting that a PVC is down; default value is 5
- retryFrequency—Number of seconds, in the range 1–600, for the router to wait between the transmission of loopback cells when it is verifying the state of the PVC; default value is 1

#### Mode

ATM VC Configuration, ATM VC Class Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]