[Contents] [Prev] [Next] [Index] [Report an Error]

# show atm subinterface

#### Syntax

show atm subinterface
[ summary | atm interfaceSpecifier | summary atm interfaceSpecifier |
status operatingStatus ] [ filter ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Displays the current state of all ATM subinterfaces that you specify.

#### Options

- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- summary—Specifies that summary information is displayed
- status—Displays information only for the ATM subinterfaces with the specified operating status
- operatingStatus—One of the following operating states:
  - dormant
  - dormantLockout
  - down
  - lowerLayerDown
  - notPresent
  - up
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec

#### Related Topics

- Configuring an MPLS Pseudowire with VCC Cell Relay Encapsulation and Monitoring ATM Subinterfaces for Layer 2 Services over MPLS in the JUNOSe BGP and MPLS Configuration Guide

[Contents] [Prev] [Next] [Index] [Report an Error]