[Contents] [Prev] [Next] [Index] [Report an Error]

# area range

#### Syntax

For OSPFv2:

[ no ] area { areaId | areaIdInt } range ipAddress mask [ do-not-advertise ]
[ cost costValue ]

For OSPFV3:

[ no ] area { areaId | areaIdInt } range ipv6Prefix/ipv6PrefixLength
[ do-not-advertise | advertise | cost costValue ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.
cost keyword and costValue variable for OSPFv2 added in JUNOSe Release 8.1.0.

#### Description

Aggregates routes at an area boundary. By default, the range of configured networks is advertised in type 3 (summary) LSAs. The no version disables this function.

#### Options

- areaId—OSPF area ID in IP address format
- areaIdInt—OSPF area ID as a decimal value in the range 0–4294967295
- ipAddress—IP address to match
- mask—IP address mask
- ipv6Prefix—IPv6 network number to match
- ipv6PrefixLength—Length of the IPv6 prefix; a decimal value that indicates how many of the higher-order contiguous bits of the IPv6 address make up the prefix (the network portion of the IPv6 address). A slash (/) must precede this value.
- do-not-advertise—Specifies that the range of configured networks is not advertised
- advertise—Specifies that the range of configured networks is advertised (IPv6 only)
- costValue—Cost value for the specified range of networks in the range 0–65535

#### Mode

Router Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]