> - Download PDFs
> - radius remote-circuit-id-delimiter

> # radius remote-circuit-id-delimiter

> #### Syntax

> radius remote-circuit-id-delimiter delimiter

> no radius remote-circuit-id-delimiter

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.

> #### Description

> Specifies the delimiter character that sets off components in the PPPoE remote circuit ID value sent from a DSLAM and captured on the router. The no version restores the default delimiter character, #.

> #### Options

> - delimiter—Special character (for example, ! or %) to set off components in the PPPoE remote circuit ID value captured from a DSLAM; the default delimiter character is #

> #### Mode

> Global Configuration

> #### Updated: 2009-04-17

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.