[Contents] [Prev] [Next] [Index] [Report an Error]

## Pass Through RADIUS Attributes

Table 51 describes the RADIUS attribute that is not processed by JUNOSe software. The router simply passes this attribute to its destination.

Table 51: RADIUS Attribute Passed Through by JUNOSe Software

Standard Number | Attribute Name | Description
--- | --- | ---
[79] | EAP-Message | Used by RADIUS relay servers Passed through to the RADIUS server

[Contents] [Prev] [Next] [Index] [Report an Error]