[Contents] [Prev] [Next] [Index] [Report an Error]

# aps unidirectional

#### Syntax

[ no ] aps unidirectional

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Configures the APS/MSP group to operate in unidirectional mode, the default setting. The no version configures the APS/MSP group to operate in bidirectional mode.

#### Mode

Controller Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]