[Contents] [Prev] [Next] [Index] [Report an Error]

# ip ospf dead-interval

#### Syntax

ip ospf dead-interval deadInterval

no ip ospf dead-interval

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Sets the time period during which the router's neighbors do not see hello packets before they declare the router to be down. The no version resets the dead interval to its default.

#### Options

- deadInterval—Number in the range 0–2147483647 seconds; default value is 40 seconds

#### Mode

Interface Configuration, Subinterface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]