[Contents] [Prev] [Next] [Index] [Report an Error]

# ipv6 mld query-interval

#### Syntax

ipv6 mld query-interval seconds

no ipv6 mld query-interval

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Sets how often the router sends MLD host-query packets from this interface. The no version restores the default value, 125 seconds.

#### Options

- seconds—Polling interval in the range 0–65535 seconds

#### Mode

Interface Configuration, Profile Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]