[Contents] [Prev] [Next] [Index] [Report an Error]

# slot enable

#### Syntax

slot enable slotNum [ subsystem ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Enables the module installed in the specified slot. You cannot use this command on a slot that contains a primary SRP module. There is no no version.

#### Options

- slotNum—Number of the selected slot in the router; for ERX-7xx models, a number in the range 0–6; for ERX-14xx models, a number in the range 0–13; for the ERX-310 router, a number in the range 1–2; for the E120 router, a number in the range 0–5; for the E320 router, a number in the range 0–16
- subsystem—Type of subsystem on the E320 router; use when the specified slotNumber is a slot that contains an SRP module
  - srp—Indicates the SC on one or both SRP modules; specify this keyword to enable only the portion of the SC on the individual SRP module
  - fabric—Indicates the portion of the switch fabric on the SRP modules; specify this keyword to enable only an individual fabric slice

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]