[Contents] [Prev] [Next] [Index] [Report an Error]

# ip vrrp priority

#### Syntax

ip vrrp vrid priority priorityValue

no ip vrrp vrid priority

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Configures the priority of VRRP routers. The no version restores the default value, 100.

#### Options

- vrid—VRID identifier; a number in the range 1–255
- priorityValue—Priority value of the VRRP router; a number in the range 1–255; default value is 100

#### Mode

Interface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]