[Contents] [Prev] [Next] [Index] [Report an Error]

# resource if-type

#### Syntax

[ no ] resource if-type { atm-active-sub-if | atm-sub-if | atm-vc | ip | ppp-link }
{ slot slot | system }
threshold { falling fallingValue | hold-down-time holdDownTime | rising
risingValue }

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies threshold values for specific interface types on a slot or systemwide basis. The no version sets the threshold parameter to its default value (for rising, 90% of the maximum value of the resource; for falling, 1% of the maximum value of the resource; for hold-down time, 300 seconds).

| Caution: Do not specify a falling value larger than the specified rising value; do not specify a rising value smaller than the specified falling value.

#### Options

- atm-active-sub-if—Configures active ATM subinterfaces
- atm-sub-if—Configures both active and inactive ATM subinterfaces
- atm-vc—Configures ATM virtual circuits
- ip—Configures IP interfaces
- ppp-link—Configures PPP link interfaces
- slot—Number of the chassis slot in the range 0–2 (ERX-310 model), 0–6 (ERX-7xx models), 0–13 (ERX-14xx models), 0–5 (E120 router), and 0-16 (E320 router)
- For ERX-7xx models, a number in the range 0–6; for ERX-14xx models, a number in the range 0–13; for the ERX-310 router, a number in the range 1–2; for the E120 router, a number in the range 0–5; for the E320 router, a number in the range 0–16
- fallingValue—Falling threshold for the resource, in the range 0–4294967295
- holdDownTime—Hold-down time for the resource, in the range 0–4294967295 seconds
- risingValue—Rising threshold for the resource, in the range 0–4294967295

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]