[Contents] [Prev] [Next] [Index] [Report an Error]

# mpls classifier-list

#### Syntax

mpls classifier-list classifierName
[ traffic-class className ] [ color { green | yellow | red } ]
[ user-packet-class userPacketClassValue ] [ exp-bits expValue
[ exp-mask maskValue ]

no mpls classifier-list classifierName [ classifierNumber ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Creates or modifies an MPLS classifier control list. The no version deletes the MPLS classifier control list.

#### Options

- classifierName—Name of a classifier list entry
- className—Name of a traffic class; the router supports up to eight traffic classes
- green—Matches packet color to green, indicating a low drop preference
- yellow—Matches packet color to yellow, indicating a medium drop preference
- red—Matches packet color to red, indicating a high drop preference
- userPacketClassValue—Value of the user packet class in the range 0–15
- expValue—Value of the EXP bits in the range 0–7
- maskValue—Mask applied to the EXP bits in the range 1–7
- classifierNumber—Index of the classifier control list entry to be deleted; an integer in the range 1–10000

#### Mode

Global Configuration

#### Related Topics

- Creating or Modifying Classifier Control Lists for MPLS Policy Lists

[Contents] [Prev] [Next] [Index] [Report an Error]