[Contents] [Prev] [Next] [Index] [Report an Error]

# domain-tag

#### Syntax

domain-tag routeTag

no domain-tag

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Sets the VPN route tag for an OSPF VRF on a PE to prevent routing loops back into the VPN. The no version restores the default value.

#### Options

- routeTag—Number identifying the VPN route tag in the range 0–4294967295

#### Mode

Router Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]