[Contents] [Prev] [Next] [Index] [Report an Error]

# ip dvmrp accept-filter

#### Syntax

[ no ] ip dvmrp accept-filter listName1 [ distance ] neighbor-list listName2

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Filters incoming DVMRP reports in accordance with a standard IP access list. The no version disables the filter.

#### Options

- listName1—Name of the IP access list. If the name is 0, the interface accepts all destinations. You can specify a simple or extended access list; with an extended access list you can specify an address and a subnet mask.
- distance—Number in the range 0–255; default value is 0; the distance associated with the DVMRP route when the router determines the RPF interface for the source of a multicast packet
- listName2—Name of an access list containing the neighbors from which the router will accept reports. If the name is 0, the interface accepts destinations from all its neighbors.

#### Mode

Interface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]