[Contents] [Prev] [Next] [Index] [Report an Error]

# ip rsvp signalling hello

#### Syntax

{ ip | mpls } rsvp signalling hello
[ refresh { interval helloInterval | misses helloMisses } ]

{ no | default } { ip | mpls } rsvp signalling hello

#### Description

Turns on or configures RSVP-TE hello support. See the mpls rsvp signalling hello command for a complete description and syntax.

#### Mode

Global Configuration, Interface Configuration, Subinterface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]