[Contents] [Prev] [Next] [Index] [Report an Error]

# Overview

The IP security functionality covered in this chapter includes the following major areas:

- Encapsulating protocols, including authentication (AH) and Encapsulating Security Payload (ESP), to provide security on specified packets
- The Internet Security Association and Key Management Protocol/Internet Key Exchange (ISAKMP/IKE) protocol suite to provide automatic negotiation of security associations, including session keys

## IPSec Terms and Acronyms

Table 8 describes terms and abbreviations that are used in this discussion of IPSec.

Table 8: IPSec Terms and Abbreviations

Term or Abbreviation | Description
--- | ---
3DES | Triple DES encryption/decryption algorithm
AH | Authentication header. Provides authentication of the sender and of data integrity.
CA | Certificate authority
DES | Data Encryption Standard encryption algorithm
DPD | Dead peer detection, which enables router to detect when communication to remote peer has been disconnected. Also known as IKE keepalive.
DSS | Digital Signature Standard authentication algorithm
ESP | Encapsulating Security Payload, which provides data integrity, data confidentiality and, optionally, sender's authentication
FQDN | Fully qualified domain name, which consists of the hostname and domain name for a specific system
HMAC | Hashed Message Authentication Code
IKE | Internet Key Exchange
IKE endpoint | IP address of the entity that is one of two endpoints in an IKE/ISAKMP SA.
Inbound traffic | In the context of a secure interface, already secured traffic arriving on that interface (identified based on its SPI). This traffic is cleared and checked against the security parameters set for that interface.
IPSec | Internet Protocol Security
IPSec endpoint | IP address of the entity that is one of two endpoints in an IPSec SA
ISAKMP | Internet Security Association and Key Management Protocol
ISAKMP SA | Security associations used to secure control channels between security gateways. These are negotiated via IKE phase 1.
MDx | Message Digest hash algorithm
Nonce | A random value used to detect and protect against replay attacks
Outbound traffic | In the context of a secure interface, the clear traffic forwarded to the interface (either by policy or by routing) that is typically secured according to security parameters set for that interface.
PFS | Perfect forward secrecy
RSA | Rivest-Shamir-Adleman encryption algorithm
SA | Security association. The set of security parameters that dictate how IPSec processes a packet, including encapsulation protocol and session keys. A single secure tunnel uses multiple SAs.
Secure tunnel | A virtual connection between two security gateways used to exchange data packets in a secure way. A secure tunnel is made up of a local SA and a remote SA, where both are negotiated in the context of an ISAKMP SA.
SHA | Secure Hash Algorithm
SPI | Security parameter index
VPN | Virtual private network

[Contents] [Prev] [Next] [Index] [Report an Error]