[Contents] [Prev] [Next] [Index] [Report an Error]

# Upper-Layer Protocols over Static Ethernet Platform Considerations

You can configure upper-layer protocols over Ethernet on the following E-series routers:

- E120 router
- E320 router
- ERX-1440 router
- ERX-1410 router
- ERX-710 router
- ERX-705 router
- ERX-310 router

## Module Requirements

For information about the modules supported on E-series routers:

- See the ERX Module Guide for modules supported on ERX-7xx models, ERX-14xx models, and the ERX-310 router.
- See the E120 and E320 Module Guide for modules supported on the E120 router and the E320 router.

## Interface Specifiers

The configuration task examples in this chapter use the format for ERX-7xx models, ERX-14xx models, and the ERX-310 router to specify a VLAN or S-VLAN subinterface.

For ERX-7xx models, ERX-14xx models, and ERX-310 routers, use the slot/port[.subinterface ] format. For example, the following command specifies a VLAN subinterface configured on port 0 of an I/O module in slot 4.

`

host1(config)#interface fastEthernet 4/0.1

`

For E120 and E320 routers, use the slot/adapter/port[.subinterface ] format, which includes an identifier for the bay in which the I/O adapter (IOA) resides. For example, the following command specifies a VLAN subinterface configured on port 0 of the IOA installed in the upper adapter bay of slot 3.

`

host1(config)#interface gigabitEthernet 3/0/0.1

`

For more information about interface types and specifiers on E-series models, see Interface Types and Specifiers in JUNOSe Command Reference Guide.

[Contents] [Prev] [Next] [Index] [Report an Error]