[Contents] [Prev] [Next] [Index] [Report an Error]

# atm atm1483 auto-configure

#### Syntax

atm atm1483 auto-configure upperInterfaceType
[ lockout-time { minValue maxValue | none } ]

no atm atm1483 auto-configure upperInterfaceType [ lockout-time ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies one or more types of dynamic upper interface encapsulations that are accepted or detected by a dynamic ATM 1483 subinterface. Optionally, specifies the lockout time range for the encapsulation type. You can issue this command repeatedly in Profile Configuration mode to include autodetection of multiple upper interface encapsulation types within the base profile for a dynamic ATM 1483 subinterface. The no version terminates detection of the specified encapsulation type.

| Note: Encapsulation type lockout is available for bridged Ethernet, IP, PPP, and PPPoE encapsulation types.

#### Options

- upperInterfaceType—One of the following dynamic encapsulation types:
  - bridgedEthernet
  - ip
  - ppp
  - pppoe
- minValue—Minimum lockout time in the range 1–86400 seconds (24 hours); default value is 1 second
- maxValue—Maximum lockout time in the range 1–86400 seconds (24 hours); default value is 300 seconds (5 minutes)
- none—Disables lockout for the specified dynamic encapsulation type

#### Mode

Profile Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]