[Contents] [Prev] [Next] [Index] [Report an Error]

## Example: Configuring CLI-Based Interface-Specific Mirroring

This example shows the configuration of a CLI-based packet mirroring session for a particular static IP interface. The configuration results in all traffic through the interface being replicated and the replicated traffic then sent through an IPSec tunnel to the analyzer device.

1. Enable the visibility and use of the packet mirroring CLI commands.
   `
   host1#mirror-enable
   `
2. Configure the analyzer interface and a route to reach the analyzer device at 192.168.125.29.

   | Note: If the analyzer interface is Ethernet-based, you must configure a static ARP entry for the analyzer device.

   `
   host1(config)#virtual-router vr1
   host1:vr1(config)#interface tunnel ipsec:Diag transport-virtual-router default
   host1:vr1(config-if)#ip analyzer
   host1:vr1(config-if)#exit
   host1:vr1(config)#ip route 192.168.125.29 255.255.255.255 tunnel ipsec:Diag
   `
3. Configure the secure IP policy that forwards the mirrored traffic to the analyzer device at 192.168.125.29.

   In this example, the configured mirror rule does not include the analyzer-udp-port keyword. Therefore, the rule sets the mirror header to disable, which means that the mirror header is not prepended to the mirrored packets. See Understanding the Prepended Header During a Packet Mirroring Session for information about the prepended mirror header. The classifier-group command uses a previously configured classifier list, secClassA.

   `
   host1:vr1(config)#secure ip policy-list secureIpPolicy1
   host1:vr1(config-policy-list)#classifier-group secClassA
   host1:vr1(config-policy-list-classifier-group)#mirror analyzer-ip-address 192.168.125.29 analyzer-virtual-router vr1
   `
4. Attach the secure policy to the interfaces whose traffic you want to mirror. This example mirrors input traffic at interface ATM 5/0.1 and output traffic at interface ATM 5/0.2.
   `
   host1:vr1(config)#interface atm 5/0.1
   host1:vr1(config-if)#ip policy secure-input secureIpPolicy1
   host1:vr1(config)#interface atm 5/0.2
   host1:vr1(config-if)#ip policy secure-output secureIpPolicy1
   `
5. Verify the secure policy configuration.

       host1# show secure policy-list name secureIpPolicy1
                                         Policy Table
                                         ------ -----
       Secure IP Policy secureIpPolicy1
        Administrative state: enable
        Reference count:      2
        Classifier control list: secClassA
         mirror analyzer-ip-address 192.168.125.29 analyzer-virtual-router vr1
        Referenced by interface(s):
         ATM5/0.1  secure-input policy, virtual-router vr1
         ATM5/0.2  secure-output policy, virtual-router vr1

[Contents] [Prev] [Next] [Index] [Report an Error]