> - Download PDFs
> - debounce-interval

> # debounce-interval

> #### Syntax

> debounce-interval seconds

> no debounce-interval

> #### Release Information

> Command introduced in JUNOSe Release 9.3.0.

> #### Description

> Modifies the minimum time an Ethernet interface must maintain a given state—for example, up or down—before the interface notifies the upper-layer protocols of the state change. The no version restores the default value, 1 second.

> | Note: You can configure this command only if you have enabled the debounce timer feature using the debounce command.

> #### Options

> - seconds—Interval for which an interface must maintain a given state before the interface reports the state change to the upper-layer protocols. Number in the range 1–5 seconds; default value is 1 second.

> #### Mode

> Interface Configuration

> #### Updated: 2009-04-22

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.