[Contents] [Prev] [Next] [Index] [Report an Error]

# Enabling Source Address Validation

Source address validation verifies that a packet has been sent from a valid source address. When a packet arrives on an interface, the router performs a routing table lookup using the source address. The result from the routing table lookup is an interface to which packets destined for that address are routed. This interface must match the interface on which the packet arrived. If it does not match, the router drops the packet.

| Caution: When the routing table lookup for a source address contains an ECMP route, the router returns a list of interfaces for multiple next-hops. One of the interfaces in this list must match the interface on which the packet arrived or the router drops the packet. If the ECMP route uses indirect next-hops, the returned list of interfaces does not include interfaces that are reachable by those indirect next-hops. For example, if a packet arrives on an interface with source address validation enabled, and the interface is represented only by an indirect next-hop, a match for that interface does not appear in the list of interfaces from the routing table lookup. The router drops the packet.

ipv6 sa-validate

- Use to enable source address validation. Source address validation verifies that a packet has been sent from a valid source address.
- Example
  `
  host1(config-if)#ipv6 sa-validate
  `
- Use the no version to disable source address validation.
- See ipv6 sa-validate

[Contents] [Prev] [Next] [Index] [Report an Error]