[Contents] [Prev] [Next] [Index] [Report an Error]

# auto-configure

#### Syntax

auto-configure upperInterfaceType [ lockout-time { minValue maxValue | none } ]

no auto-configure upperInterfaceType [ lockout-time ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies the type(s) of dynamic encapsulations that are accepted or detected by the static ATM 1483 interface. Optionally, specifies the lockout time range for the encapsulation type. You can enter this command repeatedly in Subinterface Configuration mode. The no version terminates detection of the specified encapsulation type or, if the lockout-time keyword is specified, restores the lockout time range to its default values.

| Note: Encapsulation type lockout is available for bridged Ethernet, IP, PPP, and PPPoE encapsulation types.

#### Options

- upperInterfaceType—One of the following dynamic encapsulation types:
  - bridgedEthernet
  - ip
  - ppp
  - pppoe
- minValue—Minimum lockout time in the range 1–86400 seconds (24 hours); default value is 1 second
- maxValue—Maximum lockout time in the range 1–86400 seconds (24 hours); default value is 300 seconds (5 minutes)
- none—Disables lockout for the specified dynamic encapsulation type

#### Mode

Interface Configuration, Subinterface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]