[Contents] [Prev] [Next] [Index] [Report an Error]

# ip igmp ssm-map enable

#### Syntax

[ no ] ip igmp ssm-map enable

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Enables SSM mapping on the router. SSM mapping statically assigns sources to IGMPv1 and IGMPv2 groups. You must use SSM mapping for IGMPv1 and IGMPv2 hosts to interoperate with PIM SSM. SSM mapping allows the router to use a statically configured list to translate (*,G) memberships to (S,G) memberships. The no version disables the SSM map.

#### Mode

Privileged Exec, User Exec

[Contents] [Prev] [Next] [Index] [Report an Error]