[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring RSVP-TE Hellos Based on Node IDs

You can configure the exchange of node-ID–based RSVP-TE hellos (node hellos) for interoperability with routers that cannot support RSVP-TE graceful restart with link-based hellos. E-series routers use node hellos only to support their graceful restart capabilities.

| Note: Graceful restart must be enabled on the VR so that the node hellos can advertise the graceful restart capabilities. Link-based hellos are not required for graceful restart when you have configured node hellos. However, you might still use link-based hellos to monitor RSVP-TE links and detect link failures.

To configure the exchange of RSVP-TE node hellos on all RSVP-TE interfaces in the VR:

1. Enable RSVP-TE graceful restart.
   `
   host1:vr5(config)#mpls rsvp signalling hello graceful-restart
   `
2. Enable node hellos.
   `
   host1:vr5(config)#mpls rsvp signalling node-hello
   `
3. (Optional) Configure the refresh interval.
   `
   host1(config-if)#mpls rsvp signalling node-hello refresh interval 12000
   `
4. (Optional) Configure the refresh misses.
   `
   host1(config-if)#mpls rsvp signalling node-hello refresh misses 5
   `

   | Note: Issuing the refresh interval or the refresh misses keywords only configures the refresh values; this action has no effect on enabling or disabling RSVP-TE node hellos.

#### Related Topics

- Basic MPLS Configuration Tasks
- Additional RSVP-TE Configuration Tasks
- mpls rsvp signalling node-hello

[Contents] [Prev] [Next] [Index] [Report an Error]