[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring Active Owner Sessions with Service Manager

#### Purpose

Display information about active subscriber sessions, by owner.

#### Action

To display summary information for all active owner sessions:

    host1# show service-management owner-session brief
                                 Subscriber Sessions
                                 -------------------
                                                                           Service
       Name          Interface      Id  Owner/Id     State   Non-volatile  Sessions
    ---------------- -------------- --  ---------    ------ ------------  --------
    CLIENT1@ISP.COM   ip192.168.0.3  1  AAA 4194326  Active  False         1
    CLIENT2@ISP.COM   ip192.168.0.7  2  AAA 4194327  Active  False         1
    CLIENT3@ISP.COM   ip192.168.0.4  3  AAA 4194328  Active  False         1
    CLIENT4@ISP.COM   ip192.168.0.5  4  AAA 4194329  Active  False         1
    CLIENT5@ISP.COM   ip192.168.0.6  5  AAA 4194330  Active  False         1
    CLIENT6@ISP.COM   ip192.168.0.8  6  AAA 4194331  Active  False         1
    CLIENT7@ISP.COM   ip192.168.0.1  7  AAA 4194332  Active  False         1
    CLIENT8@ISP.COM   ip192.168.0.9  8  AAA 4194333  Active  False         1

To display information for a particular owner:

    host1# show service-management owner-session aaa 4194326
    User Name: CLIENT1@ISP.COM, Interface: ip 192.168.0.1
     Owner/Id: AAA/4194326
     Non-volatile: False
     State: Active
     ServiceSessions:
             Name             Owner/ID      State                 Operation
    -----------------------   -----------   -------------------   ---------
    tiered(2000000,3000000)   AAA 4194326   Config ApplySuccess   Activate
             Name             Non-volatile
    -----------------------   ------------
    tiered(2000000,3000000)   False

To display information for a particular owner with service session information:

    host1# show service-management owner-session aaa 4194326 service-session
    User Name: client1@isp.COM, Interface: ip192.168.0.1
    Service : tiered(2000000,3000000)
     Non-volatile : False
     Owner : AAA 4194326
     State : Config ApplySuccess
     Activate : True
     Statistics Type : time-based and volume-based
     Statistics Complete : False
     Poll Interval : 0
     Poll Expire : 0
     Activate Time : THU MAR 02 01:21:26 2006
     Time : 0
     Time Expire : 0
     Volume MBytes: 2
     Volume Expire MBytes : 1
     Input Bytes : 594
     Output Bytes : 1196
     Input Packets : 1
     Output Packets : 2

#### Meaning

Table 159 lists the show service-management owner-session command output fields.

Table 159: show service-management owner-session Output Fields

Field Name | Field Description
--- | ---
Name | Name of the subscriber or name of the service session
Interface | Type and IP address of the subscriber’s interface
Owner/Id | Method used to activate the subscriber session (CLI, AAA) and ID number generated by the owner
State | Status of the subscriber session (active or inactive), or status of the service session
Non-volatile | Indicates whether the service session is stored in NVS; RADIUS-based service sessions are not stored in NVS
Service Sessions | Number of service sessions currently active for this subscriber
Operation | Last operation that Service Manager performed
Service | Name of the service, with parameter values in parentheses
Activate | Indicates whether the last operation was activate (True) or deactivate (False)
Statistics Type | Type of statistics collected; none, time, or volume-time
Statistics Complete | Whether statistics have been successfully collected; True or False
Poll Interval | Interval, in seconds, that interim statistics reports are sent
Poll Expire | Number of seconds until the next statistics report is sent
Activate Time | Day, date, and time when the service session was activated
Time | Time threshold value set by service session profile or RADIUS VSA
Time Expire | Time left until the threshold expires; this value starts as the time threshold value and is decremented as time passes
Volume | Volume threshold value set by service session profile or RADIUS VSA
Volume Expire | Volume left until the threshold is exceeded; this value starts as the volume threshold value and is decremented as the service statistics measure volume
Input Bytes | Current value of input bytes that the statistics configuration is measuring
Output Bytes | Current value of output bytes that the statistics configuration is measuring
Input Packets | Current value of input packets that the statistics configuration is measuring
Output Packets | Current value of output packets that the statistics configuration is measuring

#### Related Topics

- show service-management owner-session

[Contents] [Prev] [Next] [Index] [Report an Error]