[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring Configured Destination Profiles or Host Profiles

#### Purpose

Display either a list of configured L2TP destination profiles or the host profiles defined in a particular profile.

If a nondefault L2TP RWS is configured for a particular host profile, the command displays the RWS setting as an attribute of that host profile. (See Example 2.)

#### Action

To display either a list of configured L2TP destination profiles or the host profiles defined in a particular profile:

    host1#show l2tp destination profile
    L2TP destination profile westford
    1 L2TP destination profile found

If a nondefault L2TP RWS is configured for a particular host profile, to display the RWS setting as an attribute of that host profile:

    host1#show l2tp destination profile westford
    L2TP destination profile westford
    Configuration
      Destination address
        Transport ipUdp
        Virtual router lns
        Peer address 192.168.1.99
      Destination profile maximum sessions is 5000
    Statistics
      Destination profile current session count is 2
    Host profile attributes
      Remote host is remhost22.xyz.com
        Configuration
          Tunnel password is 23erf5
          Interface profile is ebcints
          Bundled group id is 1
          Bundled group id override is enabled
          Maximum sessions is 400
          Failover resync is failover-protocol
        Statistics
          Current session count is 14
      Remote host is asciitext
        Configuration
          Bundled group id is 0
          Tunnel password is 222
          Interface profile is ascints
          Default upper binding type mlppp
          Maximum sessions is 250
          Failover resync is failover-protocol
        Statistics
          Current session count is 2
      Remote host is mexico
        Configuration
          Local ip address is 10.10.2.2
          Proxy lcp is disabled
          Proxy authenticate is enabled
          mlppp upper binding type
          Disconnect-cause avp is enabled
          Receive window size is 4
          Maximum sessions is 500
          Failover resync is failover-protocol
        Statistics
          Current session count is 14
      Remote host is LAC
        Configuration
          Tunnel password is TunnelPass
          Local host name is LNS
          Local ip address is 46.1.1.2
          Disconnect-cause avp is enabled
          Tunnels are single-shot
          Override out-of-resource-result-code is enabled
        Statistics
          Current session count is 0
    5 L2TP host profiles found

#### Meaning

Table 85 lists the show l2tp destination profile command output fields.

Table 85: show l2tp destination profile Output Fields

Field Name | Field Description
--- | ---
Destination profile attributes | Destination profile attributes of L2TP destination
Transport | Method used to transfer traffic
Virtual Router | Method used to transfer traffic
Peer address | IP address of the LAC
Destination profile maximum sessions | Maximum number of sessions allowed for the destination profile
Destination profile current session count | Number of current sessions for the destination profile
Host profile attributes | Host profile attributes of L2TP destination
Remote host | Name of the remote host
Local hostname | Name of the local host
Local IP address | IP address of the local host
Bundled group id | Identifier for bundled sessions
Tunnel password | Password for the tunnel
Interface profile | Name of the host profile
Proxy lcp | Status of proxy LCP for the remote host
mlppp upper binding type | Default upper binding type
Disconnect-cause avp generation | Status of the disconnect cause generation
Receive window size | Number of packets that the peer can transmit without receiving an acknowledgment from the router
Maximum sessions | Maximum number of sessions allowed for the host profile
Failover resync | L2TP peer resynchronization method for the host profile
Override out-of-resource-result-code | State of result code override, enabled or disabled
Current session count | Number of current sessions for the host profile

#### Related Topics

- show l2tp destination profile

[Contents] [Prev] [Next] [Index] [Report an Error]