[Contents] [Prev] [Next] [Index] [Report an Error]

# ip ospf priority

#### Syntax

ip ospf priority intfPriority

no ip ospf priority

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Sets the router priority. Used in determining the designated router for the particular network. This designation applies only to multiaccess networks. Every broadcast and nonbroadcast multiaccess network has a designated router. The no version restores the default value.

#### Options

- intfPriority—Priority value, an 8-bit number in the range 1–255; default value is 1

#### Mode

Interface Configuration, Subinterface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]