[Contents] [Prev] [Next] [Index] [Report an Error]

# tunnel mpls retry-time

#### Syntax

tunnel mpls [ no-route ] retry-time retryTime

no tunnel mpls retry-time

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies for a particular tunnel the interval in seconds between attempts to set up an LSP for RSVP-TE after a failure other than one due to no available route. The no version restores the default value, 5 seconds.

#### Options

- retryTime—Number of seconds in the range 1–60

#### Mode

Interface Configuration, Tunnel Profile Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]