[Contents] [Prev] [Next] [Index] [Report an Error]

## ospfHelloPktsRcvd

#### Description

Processing of hello messages received on OSPF-enabled interfaces

#### Emergency

None

#### Alert

None

#### Critical

None

#### Error

None

#### Warning Log

Invalid packet, hello parameters mismatch (area, network, hello and dead intervals, version, md5 digest)

#### Notice Log

None

#### Info

None

#### Debug

Received hello information (ip source/destination, length)

#### Filter

router virtualRouterName [ interface interfaceType interfaceSpecifier ]

- router—Logs events for a specific virtual router
- virtualRouterName—Name of the virtual router for which you want to log events
- interface—Logs events on a specific OSPF-enabled interface on the virtual router
- interfaceType—Type of the interface for which you want to log events (for example, atm or fastEthernet)
- interfaceSpecifier—Location of the interface in the appropriate format

  | Note: For information about interface types and specifiers, see Interface Types and Specifiers in JUNOSe Command Reference Guide.

[Contents] [Prev] [Next] [Index] [Report an Error]