[Contents] [Prev] [Next] [Index] [Report an Error]

# show radius override

#### Syntax

show radius override [ filter ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Displays the current override settings configured on the RADIUS client (LNS) for the NAS-IP-Address [4], NAS-Port-Id [87], Calling-Station-Id [31], and NAS-Identifier [32] RADIUS attributes. The nas-info field in the command output indicates the virtual router that generates the NAS-IP-Address and NAS-Identifier attributes for AAA broadcast accounting packets.

#### Options

- filter—See Filtering show Commands

#### Mode

Privileged Exec

[Contents] [Prev] [Next] [Index] [Report an Error]