[Contents] [Prev] [Next] [Index] [Report an Error]

# snmp-server security

#### Syntax

snmp-server security { no-access | read | read-write }

no snmp-server security

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies a security access level for the SNMP agent. The no version returns the SNMP security level to its default, no access.

#### Options

- no-access—Specifies that no other virtual routers can access this router for read or write actions
- read—Specifies that other virtual routers can access this router for read only actions
- read-write—Specifies that other virtual routers can access this router for both read and write actions

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]