[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring Rate-Limit Profiles

#### Purpose

Display information about rate-limit profiles.

#### Action

To display information about rate-limit profiles:

    host1#show rate-limit-profile
                                Rate Limit Profile Table
                                ---- ----- ------- -----
    IP Rate-Limit-Profile: rlp
       Profile Type:                   one-rate
       Reference count:                0
       Committed rate:                 0
       Committed burst:                8192
       Excess burst:                   0
       Mask:                           255
       Committed rate action:          transmit
       Conformed rate action:          transmit
       Exceeded rate action:           drop
    IP Rate-Limit-Profile: rlp
       Profile Type:                   two-rate hierarchical
       Color-aware                     no
       Reference count:                0
       Committed rate:                 0
       Committed burst:                8192
       Peak rate:                      0
       Peak burst:                     8192
       Mask:                           255
       Committed rate action:          transmit unconditional
       Conformed rate action:          transmit conditional
       Exceeded rate action:           drop
    L2TP Rate-Limit-Profile: L2tpRlp
       Profile Type:                   two-rate
       Reference count:                0
       Committed rate:                 0
       Committed burst:                8192
       Peak rate:                      0
       Peak burst:                     8192
       Committed rate action:          transmit
       Conformed rate action:          transmit
       Exceeded rate action:           drop

#### Meaning

Table 39 lists the show rate-limit-profile command output fields.

Table 39: show rate-limit-profile Output Fields

Field Name | Field Description
--- | ---
Rate-Limit-Profile | Create a rate limit profile
Profile Name | Name of the rate-limit profile
Profile Type | One-rate, two-rate, or hierarchical profile
Reference count | Number of policy lists that reference this rate-limit profile
Color-aware | Color-aware action (yes or no) taken for profile
Committed rate | Target rate for the traffic, in bits per second
Committed burst | Amount of bandwidth allocated to accommodate bursty traffic, in bytes
Excess burst | Amount of bandwidth allocated to accommodate a packet in progress when the rate is in excess of the burst, in bytes
Peak rate | Amount of bandwidth allocated to accommodate traffic flow in excess of the committed rate, in bits per second
Peak burst | Amount of bandwidth allocated to accommodate bursty traffic in excess of the peak rate, in bytes
Mask | Value of mask applied to ToS byte in IP packet header
Committed rate action | Policy action (drop, transmit, or mark) taken when traffic flow does not exceed the committed rate
Conformed rate action | Policy action (drop, transmit, or mark) taken when traffic flow exceeds the committed rate but remains below the peak rate
Exceeded rate action | Policy action (drop, transmit, or mark) taken when traffic flow exceeds the peak rate

#### Related Topics

- show rate-limit-profile

[Contents] [Prev] [Next] [Index] [Report an Error]